IFC building model
Schema: "IFC4"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Project Number"
Time stamp: "2022-11-07T10:58:40"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20200210_1400(x64) - Exporter 20.2.12.1 - Default UI"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"

People and organizations
  Person "rorza" of Organization (no name given)
  Owner history of Person "rorza" of Organization (no name given) | application "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)" | change NOCHANGE | created 1667476410 (2022-11-03T11:53:30Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 23′ 13.199999″ | longitude -71° 14′ 31.199999″ | elevation above sea level 0.
    IFCBUILDING
      IFCBUILDINGSTOREY "F00" | long name "F00" | object type "Level:Floor Level" | elevation 0.
        contains 3 elements
          1 x IFCPUMP | type IFCPUMPTYPE "WPU 75E-5G" | object type "HC_Heat Pump_MEPcontent_Itho Daalderop_WPU 5G Module_NL-NL:WPU 75E-5G" | names: "HC_Heat Pump_MEPcontent_Itho Daalderop_WPU 5G Module_NL-NL:WPU 75E-5G:1316757" | material: constituents "MaterialConstituentSet" ("Color RGB 050-050-050": "Color RGB 050-050-050", "Color RAL 9006": "Color RAL 9006", "Color RGB 187-080-046": "Color RGB 187-080-046", "Color RGB 000-000-255": "Color RGB 000-000-255", "Color RGB 255-000-000": "Color RGB 255-000-000", "Color RAL 9003": "Color RAL 9003") | property sets: Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation, Pset_PumpTypeCommon, Constraints, Dimensions, Electrical - Loads
          1 x IFCPUMP | type IFCPUMPTYPE "WPV 200L 3G" | object type "HC_Heat Pump_MEPcontent_Itho Daalderop_WPV 5_Storage Tank_NL-NL-Shared:WPV 200L 3G" | names: "HC_Heat Pump_MEPcontent_Itho Daalderop_WPV 5_Storage Tank_NL-NL-Shared:WPV 200L 3G:1316758" | material: constituents "MaterialConstituentSet" ("Color RAL 9006": "Color RAL 9006", "Color RGB 050-050-050": "Color RGB 050-050-050", "Color RAL 9003": "Color RAL 9003") | property sets: Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation, Pset_PumpTypeCommon, Constraints, Dimensions, Electrical - Loads
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "WPU 5G - Onderomkasting 3G" | object type "HC_Heat Pump_Itho Daalderop_WPU 5G_Onderomkasting 3G_Shared:WPU 5G - Onderomkasting 3G" | names: "HC_Heat Pump_Itho Daalderop_WPU 5G_Onderomkasting 3G_Shared:WPU 5G - Onderomkasting 3G:1316759" | material: constituents "MaterialConstituentSet" ("Color RGB 050-050-050": "Color RGB 050-050-050", "Color RAL 9003": "Color RAL 9003", "Color RAL 9006": "Color RAL 9006") | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation, Constraints, Dimensions, Identity Data

Types
  IFCPUMPTYPE "WPU 75E-5G" | 1 occurrence | material: constituents "MaterialConstituentSet" ("Color RGB 050-050-050": "Color RGB 050-050-050", "Color RAL 9006": "Color RAL 9006", "Color RGB 187-080-046": "Color RGB 187-080-046", "Color RGB 000-000-255": "Color RGB 000-000-255", "Color RGB 255-000-000": "Color RGB 255-000-000", "Color RAL 9003": "Color RAL 9003") | property sets: Constraints, Dimensions, Electrical, Electrical - Loads, Identity Data, Materials and Finishes
  IFCPUMPTYPE "WPV 200L 3G" | 1 occurrence | material: constituents "MaterialConstituentSet" ("Color RAL 9006": "Color RAL 9006", "Color RGB 050-050-050": "Color RGB 050-050-050", "Color RAL 9003": "Color RAL 9003") | property sets: Constraints, Dimensions, Electrical - Loads, Identity Data, Materials and Finishes, Mechanical
  IFCBUILDINGELEMENTPROXYTYPE "WPU 5G - Onderomkasting 3G" | 1 occurrence | material: constituents "MaterialConstituentSet" ("Color RGB 050-050-050": "Color RGB 050-050-050", "Color RAL 9003": "Color RAL 9003", "Color RAL 9006": "Color RAL 9006") | property sets: Constraints, Identity Data, Materials and Finishes, Mechanical, Other, Pset_BuildingElementProxyCommon

Property sets
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Floor Level" (IFCTEXT)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "GE_tag_level_floor_MEPcontent: standard" (IFCLABEL)
    Symbol at End 1 Default = TRUE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Pset_EnvironmentalImpactIndicators | properties | on 1 object (1 IFCPUMP) | on 1 type object
    Reference = "WPU 75E-5G" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 1 object (1 IFCPUMP) | on 1 type object
    Reference = "WPV 200L 3G" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "WPU 5G - Onderomkasting 3G" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 3 objects (2 IFCPUMP, 1 IFCBUILDINGELEMENTPROXY) | on 3 type objects
    Manufacturer = "Itho Daalderop" (IFCLABEL)
  Pset_PumpTypeCommon | properties | on 1 object (1 IFCPUMP) | on 1 type object
    Reference = "WPU 75E-5G" (IFCIDENTIFIER)
  Pset_PumpTypeCommon | properties | on 1 object (1 IFCPUMP) | on 1 type object
    Reference = "WPV 200L 3G" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCPUMP)
    Elevation from Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "None" (IFCTEXT)
    Offset from Host = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCPUMP)
    Elevation from Level = 829.999999999997 (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "None" (IFCTEXT)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset from Host = 829.999999999997 (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation from Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "None" (IFCTEXT)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset from Host = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 3 type objects
    Default Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    S4R_Use_nominal_diameter = TRUE (IFCBOOLEAN)
  Dimensions | properties | on 1 object (1 IFCPUMP)
    Area = 3.74862398016512 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.132798010690794 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    a = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Dimensions | properties | on 1 object (1 IFCPUMP)
    Area = 2.02615420965311 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.4574829730884 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 1.92497428303151 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.0373142892338742 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 type object
    Depth = 600. (IFCLENGTHMEASURE) [MILLI METRE]
    Domestic Cold Water Diameter = 22. (IFCLENGTHMEASURE) [MILLI METRE]
    Domestic Hot Water Diameter = 22. (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 830. (IFCLENGTHMEASURE) [MILLI METRE]
    Hydronic Return 1 Diameter = 22. (IFCLENGTHMEASURE) [MILLI METRE]
    Hydronic Return 2 Diameter = 22. (IFCLENGTHMEASURE) [MILLI METRE]
    Hydronic Supply 1 Diameter = 22. (IFCLENGTHMEASURE) [MILLI METRE]
    Hydronic Supply 2 Diameter = 22. (IFCLENGTHMEASURE) [MILLI METRE]
    Module Foundationplate Depth = 389.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Module Foundationplate Width = 555. (IFCLENGTHMEASURE) [MILLI METRE]
    Module Height = 611.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Width = 600. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 type object
    Depth = 600. (IFCLENGTHMEASURE) [MILLI METRE]
    Domestic Cold Water Diameter = 22. (IFCLENGTHMEASURE) [MILLI METRE]
    Domestic Hot Water Diameter = 22. (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 1272. (IFCLENGTHMEASURE) [MILLI METRE]
    Hydronic Return Diameter = 22. (IFCLENGTHMEASURE) [MILLI METRE]
    Hydronic Supply Diameter = 22. (IFCLENGTHMEASURE) [MILLI METRE]
    Width = 600. (IFCLENGTHMEASURE) [MILLI METRE]
  Electrical - Loads | properties | on 2 objects (2 IFCPUMP)
    Power = 0. (IFCPOWERMEASURE) [WATT]
  Electrical - Loads | properties | on 1 type object
    Voltage = 400. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
  Electrical - Loads | properties | on 1 type object
    Voltage = 229.999999642952 (IFCELECTRICVOLTAGEMEASURE) [VOLT]
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCPUMP)
    Casing Manufacturer Art. No. = "04-00073" (IFCTEXT)
    Connection Set Hydronic + Expansion Vessel Manufacturer Art. No. = "" (IFCTEXT)
    Connection Set Hydronic Manufacturer Art. No. = "04-00082" (IFCTEXT)
    Connection Set Tap Water Manufacturer Art. No. = "" (IFCTEXT)
    Function Code = "" (IFCTEXT)
    Mark = "4" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCPUMP)
    Function Code = "" (IFCTEXT)
    Mark = "5" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Function Code = "" (IFCTEXT)
    Mark = "6" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "F00" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Article Description = "WPU75 E-5G, 7,5 kW, kleine collectieve bron, 2 kW back-up, excl. onderomkasting" (IFCTEXT)
    Article Type = "WPU 75E-5G" (IFCTEXT)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Base Family Version = "22.07" (IFCTEXT)
    CB-NL Class = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Content Supplier URL = "www.MEPcontent.com" (IFCTEXT)
    Copyright = "© Trimble Europe BV" (IFCTEXT)
    Custom = FALSE (IFCBOOLEAN)
    Description = "WPU75 E-5G, 7,5 kW, kleine collectieve bron, 2 kW back-up, excl. onderomkasting" (IFCTEXT)
    EMCS Version = "4.0" (IFCTEXT)
    ETIM Article Class = "EC011794" (IFCTEXT)
    Family Version = "11.25" (IFCTEXT)
    GLN = "8712922000014" (IFCTEXT)
    GTIN = "8713418043232" (IFCTEXT)
    Internal Art. No. = "" (IFCTEXT)
    MEPcontent Class = "HEATPUMP" (IFCTEXT)
    Manufacturer = "Itho Daalderop" (IFCTEXT)
    Manufacturer Art. No. = "03-00582" (IFCTEXT)
    Manufacturer URL = "https://www.ithodaalderop.nl/nl-NL/professional/product/03-00582" (IFCTEXT)
    Model = "WPU 75E-5G" (IFCTEXT)
    OmniClass Number = "23.75.10.21" (IFCTEXT)
    OmniClass Title = "Heat Pumps" (IFCTEXT)
    Product Line = "Itho Daalderop" (IFCTEXT)
    Revit Version = "2020" (IFCTEXT)
    Stabu Code = "" (IFCTEXT)
    Type Name = "WPU 75E-5G" (IFCTEXT)
    URL = "https://mep.trimble.com" (IFCTEXT)
    Watermarked By = "https://mep.trimble.com" (IFCTEXT)
    Wholesaler = "" (IFCTEXT)
    Wholesaler Art. No. = "" (IFCTEXT)
  Identity Data | properties | on 1 type object
    Article Description = "WPV 200L 3G, warmtepomp voorraadvat 200L 3G" (IFCTEXT)
    Article Type = "WPV 200L 3G" (IFCTEXT)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Base Family Version = "22.12" (IFCTEXT)
    CB-NL Class = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Content Supplier URL = "www.MEPcontent.com" (IFCTEXT)
    Copyright = "© Trimble Europe BV" (IFCTEXT)
    Custom = FALSE (IFCBOOLEAN)
    Description = "WPV 200L 3G, warmtepomp voorraadvat 200L 3G" (IFCTEXT)
    EMCS Version = "4.0" (IFCTEXT)
    ETIM Article Class = "EC010184" (IFCTEXT)
    Family Version = "11.27" (IFCTEXT)
    GLN = "8712922000014" (IFCTEXT)
    GTIN = "08713418047933" (IFCTEXT)
    Internal Art. No. = "" (IFCTEXT)
    MEPcontent Class = "HEATPUMP" (IFCTEXT)
    Manufacturer = "Itho Daalderop" (IFCTEXT)
    Manufacturer Art. No. = "03-00668" (IFCTEXT)
    Manufacturer URL = "https://www.ithodaalderop.nl/nl-NL/professional/product/03-00668" (IFCTEXT)
    Model = "WPV 200L 3G" (IFCTEXT)
    OmniClass Number = "23.75.10.17.17" (IFCTEXT)
    OmniClass Title = "Combined Heating/Cooking Units" (IFCTEXT)
    Product Line = "Itho Daalderop" (IFCTEXT)
    Revit Version = "2020" (IFCTEXT)
    Stabu Code = "" (IFCTEXT)
    Type Name = "WPV 200L 3G" (IFCTEXT)
    URL = "https://mep.trimble.com" (IFCTEXT)
    Watermarked By = "https://mep.trimble.com" (IFCTEXT)
    Wholesaler = "" (IFCTEXT)
    Wholesaler Art. No. = "" (IFCTEXT)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Base Family Version = "22.12" (IFCTEXT)
    CB-NL Class = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Content Supplier URL = "www.MEPcontent.com" (IFCTEXT)
    Copyright = "© Trimble Europe BV" (IFCTEXT)
    Custom = FALSE (IFCBOOLEAN)
    Description = "WPU 5G - Onderomkasting 3G" (IFCTEXT)
    EMCS Version = "" (IFCTEXT)
    ETIM Article Class = "" (IFCTEXT)
    Family Version = "22.12" (IFCTEXT)
    GLN = "8712922000014" (IFCTEXT)
    GTIN = "08713418048633" (IFCTEXT)
    Internal Art. No. = "" (IFCTEXT)
    MEPcontent Class = "" (IFCTEXT)
    Manufacturer = "Itho Daalderop" (IFCTEXT)
    Manufacturer Art. No. = "04-00138" (IFCTEXT)
    Manufacturer URL = "https://www.ithodaalderop.nl/nl-NL/professional/product/04-00138" (IFCTEXT)
    Model = "" (IFCTEXT)
    OmniClass Number = "23.75.10.21" (IFCTEXT)
    OmniClass Title = "Heat Pumps" (IFCTEXT)
    Product Line = "Itho Daalderop" (IFCTEXT)
    Revit Version = "2020" (IFCTEXT)
    Stabu Code = "" (IFCTEXT)
    Type Name = "WPU 5G - Onderomkasting 3G" (IFCTEXT)
    URL = "https://mep.trimble.com" (IFCTEXT)
    Watermarked By = "https://mep.trimble.com" (IFCTEXT)
    Wholesaler = "" (IFCTEXT)
    Wholesaler Art. No. = "" (IFCTEXT)
  Mechanical | properties | on 1 object (1 IFCPUMP)
    System Classification = "Hydronic Return,Hydronic Supply,Domestic Hot Water,Domestic Cold Water,Power" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Mechanical | properties | on 2 type objects
    Classification = "Pump" (IFCIDENTIFIER)
  Mechanical | properties | on 1 type object
    Classification = "None" (IFCIDENTIFIER)
  Mechanical - Flow | properties | on 1 object (1 IFCPUMP)
    Domestic Cold Water Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Domestic Hot Water Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Hydronic Return Flow 1 = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Hydronic Return Flow 2 = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Hydronic Supply Flow 1 = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Hydronic Supply Flow 2 = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
  Mechanical - Flow | properties | on 1 object (1 IFCPUMP)
    Domestic Cold Water Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Domestic Hot Water Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Hydronic Return Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Hydronic Supply Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Client Name" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Project Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "Project Number" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other | properties | on 1 object (1 IFCPUMP)
    Category = "Mechanical Equipment" (IFCLABEL)
    Domestic Cold Water Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Domestic Cold Water Connection Depth = 265.7 (IFCLENGTHMEASURE) [MILLI METRE]
    Domestic Cold Water Connection Height = 794. (IFCLENGTHMEASURE) [MILLI METRE]
    Domestic Cold Water Connection Width = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Domestic Hot Water Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Domestic Hot Water Connection Depth = 205.7 (IFCLENGTHMEASURE) [MILLI METRE]
    Domestic Hot Water Connection Height = 794. (IFCLENGTHMEASURE) [MILLI METRE]
    Domestic Hot Water Connection Width = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Family = "HC_Heat Pump_MEPcontent_Itho Daalderop_WPU 5G Module_NL-NL: WPU 75E-5G" (IFCLABEL)
    Family and Type = "HC_Heat Pump_MEPcontent_Itho Daalderop_WPU 5G Module_NL-NL: WPU 75E-5G" (IFCLABEL)
    Hydronic Return 1 Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Hydronic Return 1 Connection Depth = 354. (IFCLENGTHMEASURE) [MILLI METRE]
    Hydronic Return 1 Connection Height = 747.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Hydronic Return 1 Connection Width = 300. (IFCLENGTHMEASURE) [MILLI METRE]
    Hydronic Return 2 Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Hydronic Return 2 Connection Depth = 294. (IFCLENGTHMEASURE) [MILLI METRE]
    Hydronic Return 2 Connection Height = 747.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Hydronic Return 2 Connection Width = 300. (IFCLENGTHMEASURE) [MILLI METRE]
    Hydronic Supply 1 Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Hydronic Supply 1 Connection Depth = 234. (IFCLENGTHMEASURE) [MILLI METRE]
    Hydronic Supply 1 Connection Height = 747.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Hydronic Supply 1 Connection Width = 300. (IFCLENGTHMEASURE) [MILLI METRE]
    Hydronic Supply 2 Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Hydronic Supply 2 Connection Depth = 174. (IFCLENGTHMEASURE) [MILLI METRE]
    Hydronic Supply 2 Connection Height = 747.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Hydronic Supply 2 Connection Width = 300. (IFCLENGTHMEASURE) [MILLI METRE]
    Right Domestic Cold Water Connection Safe = TRUE (IFCBOOLEAN)
    Right Domestic Hot Water Connection Safe = TRUE (IFCBOOLEAN)
    Right Hydronic Return Connection 1 Safe = TRUE (IFCBOOLEAN)
    Right Hydronic Return Connection 2 Safe = TRUE (IFCBOOLEAN)
    Right Hydronic Supply Connection 1 Safe = TRUE (IFCBOOLEAN)
    Right Hydronic Supply Connection 2 Safe = TRUE (IFCBOOLEAN)
    Show Casing-Base cabinet Safe = TRUE (IFCBOOLEAN)
    Show Casing-Frame and front panel Safe = FALSE (IFCBOOLEAN)
    Show Logo = FALSE (IFCBOOLEAN)
    Show Storage Tank = TRUE (IFCBOOLEAN)
    Storage Tank Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Storage Tank Position = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Clearance = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Cover Visibility = TRUE (IFCBOOLEAN)
    Type = "HC_Heat Pump_MEPcontent_Itho Daalderop_WPU 5G Module_NL-NL: WPU 75E-5G" (IFCLABEL)
    Type Id = "HC_Heat Pump_MEPcontent_Itho Daalderop_WPU 5G Module_NL-NL: WPU 75E-5G" (IFCLABEL)
  Other | properties | on 1 object (1 IFCPUMP)
    Category = "Mechanical Equipment" (IFCLABEL)
    Family = "HC_Heat Pump_MEPcontent_Itho Daalderop_WPV 5_Storage Tank_NL-NL-Shared: WPV 200L 3G" (IFCLABEL)
    Family and Type = "HC_Heat Pump_MEPcontent_Itho Daalderop_WPV 5_Storage Tank_NL-NL-Shared: WPV 200L 3G" (IFCLABEL)
    Storage Tank Support = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Total Height = 1272. (IFCLENGTHMEASURE) [MILLI METRE]
    Type = "HC_Heat Pump_MEPcontent_Itho Daalderop_WPV 5_Storage Tank_NL-NL-Shared: WPV 200L 3G" (IFCLABEL)
    Type Id = "HC_Heat Pump_MEPcontent_Itho Daalderop_WPV 5_Storage Tank_NL-NL-Shared: WPV 200L 3G" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Category = "Mechanical Equipment" (IFCLABEL)
    Family = "HC_Heat Pump_Itho Daalderop_WPU 5G_Onderomkasting 3G_Shared: WPU 5G - Onderomkasting 3G" (IFCLABEL)
    Family and Type = "HC_Heat Pump_Itho Daalderop_WPU 5G_Onderomkasting 3G_Shared: WPU 5G - Onderomkasting 3G" (IFCLABEL)
    Type = "HC_Heat Pump_Itho Daalderop_WPU 5G_Onderomkasting 3G_Shared: WPU 5G - Onderomkasting 3G" (IFCLABEL)
    Type Id = "HC_Heat Pump_Itho Daalderop_WPU 5G_Onderomkasting 3G_Shared: WPU 5G - Onderomkasting 3G" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: Floor Level" (IFCLABEL)
    Family and Type = "Level: Floor Level" (IFCLABEL)
    Type = "Level: Floor Level" (IFCLABEL)
    Type Id = "Level: Floor Level" (IFCLABEL)
  Other | properties | on 1 type object
    Back Clearance = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    Bottom Clearance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Category = "Mechanical Equipment" (IFCLABEL)
    Family Name = "HC_Heat Pump_MEPcontent_Itho Daalderop_WPU 5G Module_NL-NL" (IFCTEXT)
    Front Clearance = 500. (IFCLENGTHMEASURE) [MILLI METRE]
    Left Clearance = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    Right Clearance = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Cover = "HC_Heat Pump_MEPcontent_Itho Daalderop_WPV 5_Top Cover_NL-NL-Shared: Top Cover" (IFCLABEL)
  Other | properties | on 1 type object
    Back Clearance = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    Bottom Clearance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Category = "Mechanical Equipment" (IFCLABEL)
    Family Name = "HC_Heat Pump_MEPcontent_Itho Daalderop_WPV 5_Storage Tank_NL-NL-Shared" (IFCTEXT)
    Front Clearance = 500. (IFCLENGTHMEASURE) [MILLI METRE]
    Left Clearance = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    Right Clearance = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Clearance = 250. (IFCLENGTHMEASURE) [MILLI METRE]
  Other | properties | on 1 type object
    Category = "Mechanical Equipment" (IFCLABEL)
    Family Name = "HC_Heat Pump_Itho Daalderop_WPU 5G_Onderomkasting 3G_Shared" (IFCTEXT)
  Phasing | properties | on 3 objects (2 IFCPUMP, 1 IFCBUILDINGELEMENTPROXY)
    Phase Created = "4. Plan over 10 years" (IFCLABEL)
  Visibility | properties | on 1 object (1 IFCPUMP)
    Connection Set Hydronic + Expansion Vessel = FALSE (IFCBOOLEAN)
    Connection Set Hydronic = TRUE (IFCBOOLEAN)
    Connection Set Tap Water = FALSE (IFCBOOLEAN)
    Left Domestic Cold Water Connection = FALSE (IFCBOOLEAN)
    Left Domestic Hot Water Connection = FALSE (IFCBOOLEAN)
    Left Hydronic Return Connection 1 = FALSE (IFCBOOLEAN)
    Left Hydronic Return Connection 2 = FALSE (IFCBOOLEAN)
    Left Hydronic Supply Connection 1 = FALSE (IFCBOOLEAN)
    Left Hydronic Supply Connection 2 = FALSE (IFCBOOLEAN)
    Right Domestic Cold Water Connection = TRUE (IFCBOOLEAN)
    Right Domestic Hot Water Connection = TRUE (IFCBOOLEAN)
    Right Hydronic Return Connection 1 = TRUE (IFCBOOLEAN)
    Right Hydronic Return Connection 2 = TRUE (IFCBOOLEAN)
    Right Hydronic Supply Connection 1 = TRUE (IFCBOOLEAN)
    Right Hydronic Supply Connection 2 = TRUE (IFCBOOLEAN)
    Show Casing = TRUE (IFCBOOLEAN)
    Show Service Area = FALSE (IFCBOOLEAN)
    Show frame and front panel = FALSE (IFCBOOLEAN)
    Standard Connection = FALSE (IFCBOOLEAN)
    Storage Tank = "HC_Heat Pump_MEPcontent_Itho Daalderop_WPV 5_Storage Tank_NL-NL-Shared: WPV 200L 3G" (IFCLABEL)
  Visibility | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Show Casing = TRUE (IFCBOOLEAN)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "WPU 5G - Onderomkasting 3G" (IFCIDENTIFIER)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
    Reference = "Floor Level" (IFCIDENTIFIER)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
    Reference = "Project Information" (IFCIDENTIFIER)
  Electrical | properties | on 1 type object
    Hertz = 50. (IFCFREQUENCYMEASURE) [HERTZ]
    Phase = 3 (IFCINTEGER)
  Materials and Finishes | properties | on 1 type object
    Black = "Color RGB 050-050-050" (IFCLABEL)
    Blue = "Color RGB 000-000-255" (IFCLABEL)
    Connection = "Color RGB 187-080-046" (IFCLABEL)
    Light Grey = "Color RAL 9006" (IFCLABEL)
    Red = "Color RGB 255-000-000" (IFCLABEL)
    White = "Color RAL 9003" (IFCLABEL)
  Materials and Finishes | properties | on 1 type object
    Black = "Color RGB 050-050-050" (IFCLABEL)
    Light Grey = "Color RAL 9006" (IFCLABEL)
    White = "Color RAL 9003" (IFCLABEL)
  Materials and Finishes | properties | on 1 type object
    Black = "Color RGB 050-050-050" (IFCLABEL)
    Blue = "Color RGB 044-117-226" (IFCLABEL)
    Grey = "Color RGB 236-236-231" (IFCLABEL)
    Light Grey = "Color RAL 9006" (IFCLABEL)
    White = "Color RAL 9003" (IFCLABEL)
  Mechanical - Loads | properties | on 1 type object
    Cooling Power = 0. (IFCREAL)
    Heating Power = 807293.281253229 (IFCREAL)
    Operation Point Cooling = "" (IFCTEXT)
    Operation Point Heating = "" (IFCTEXT)
  Mechanical - Loads | properties | on 1 type object
    Cooling Power = 0. (IFCREAL)
    Heating Power = 0. (IFCREAL)
    Operation Point Cooling = "" (IFCTEXT)
    Operation Point Heating = "" (IFCTEXT)
  Text | properties | on 1 type object
    Pipe Type Category = "M561" (IFCTEXT)

Other addresses and roles
  2 x postal address: "Enter address here"