IFC building model
Schema: "IFC4"
Description: "ViewDefinition [CoordinationView_V2.0]"
Description: "ExchangeRequirement []"
Time stamp: "2024-12-10T18:13:25"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "22.0.2.392 - Exporter 22.0.2.392 - Default UI"
Application: "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)"

People and organizations
  Person "radu_orza" of Organization (no name given)
  Owner history of Person "radu_orza" of Organization (no name given) | application "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)" | change NOCHANGE | created 1733847205 (2024-12-10T16:13:25Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 1 element
          1 x IFCAIRTOAIRHEATRECOVERY | type IFCAIRTOAIRHEATRECOVERYTYPE "VE_Air Heater_Heat Recovery_MEPcontent_Itho Daalderop_HRU 300-375 V(EV)_NL-NL:HRU 375 EV" | object type "VE_Air Heater_Heat Recovery_MEPcontent_Itho Daalderop_HRU 300-375 V(EV)_NL-NL:HRU 375 EV" | names: "VE_Air Heater_Heat Recovery_MEPcontent_Itho Daalderop_HRU 300-375 V(EV)_NL-NL:HRU 375 EV:116609" | material: constituents "MaterialConstituentSet" ("Color RGB 135-133-129": "Color RGB 135-133-129", "Color RGB 043-043-044": "Color RGB 043-043-044", "Color RGB 236-236-231": "Color RGB 236-236-231") | property sets: Pset_AirToAirHeatRecoveryTypeCommon, Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation, Constraints, Dimensions, Electrical

Types
  IFCAIRTOAIRHEATRECOVERYTYPE "VE_Air Heater_Heat Recovery_MEPcontent_Itho Daalderop_HRU 300-375 V(EV)_NL-NL:HRU 375 EV" | 1 occurrence | material: constituents "MaterialConstituentSet" ("Equipment": "Color RGB 135-133-129", "Equipment": "Color RGB 043-043-044", "Equipment": "Color RGB 236-236-231") | property sets: Constraints, Dimensions, Electrical, Identity Data, Materials and Finishes, Mechanical

Property sets
  Pset_SiteCommon | properties | on 1 object (1 IFCSITE)
    Reference = "Project Information" (IFCIDENTIFIER)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCAIRTOAIRHEATRECOVERY)
    Bottom Clearance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Bottom Clearance Safe = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Category = "Mechanical Equipment" (IFCLABEL)
    Ceiling Mounted = FALSE (IFCBOOLEAN)
    Celing Position Safe = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Family = "VE_Air Heater_Heat Recovery_MEPcontent_Itho Daalderop_HRU 300-375 V(EV)_NL-NL: HRU 375 EV" (IFCLABEL)
    Family and Type = "VE_Air Heater_Heat Recovery_MEPcontent_Itho Daalderop_HRU 300-375 V(EV)_NL-NL: HRU 375 EV" (IFCLABEL)
    Floor Mounted Horizontal = FALSE (IFCBOOLEAN)
    Floor Mounted Vertical = TRUE (IFCBOOLEAN)
    Front Clearance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Front Clearance Safe = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Ground Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Legs Visibility = FALSE (IFCBOOLEAN)
    Horizontal Position Safe = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Left Clearance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Left Clearance Safe = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Left Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Right Clearance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Right Clearance Safe = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Service Space = FALSE (IFCBOOLEAN)
    Top Clearance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Clearance Safe = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Type = "VE_Air Heater_Heat Recovery_MEPcontent_Itho Daalderop_HRU 300-375 V(EV)_NL-NL: HRU 375 EV" (IFCLABEL)
    Type Id = "VE_Air Heater_Heat Recovery_MEPcontent_Itho Daalderop_HRU 300-375 V(EV)_NL-NL: HRU 375 EV" (IFCLABEL)
    Vertical Legs Visibility = TRUE (IFCBOOLEAN)
    Wall Bracket Visibility = FALSE (IFCBOOLEAN)
    Wall Mounted Horizontal = FALSE (IFCBOOLEAN)
    Wall Mounted Vertical = FALSE (IFCBOOLEAN)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: Level 1" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level: Level 1" (IFCLABEL)
    Type Id = "Level: Level 1" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Mechanical Equipment" (IFCLABEL)
    Ceiling Mounted 1 = "Ceiling Mounted" (IFCLABEL)
    Family Name = "VE_Air Heater_Heat Recovery_MEPcontent_Itho Daalderop_HRU 300-375 V(EV)_NL-NL" (IFCTEXT)
    Floor Horizontal = "Floor Mounted Horizontal" (IFCLABEL)
    Floor Vertical = "Floor Mounted Vertical" (IFCLABEL)
    Wall Horizontal = "Wall Mounted Horizontal" (IFCLABEL)
    Wall Vertical = "Wall Mounted Vertical" (IFCLABEL)
  Pset_AirToAirHeatRecoveryTypeCommon | properties | on 1 object (1 IFCAIRTOAIRHEATRECOVERY)
    Reference = "HRU 375 EV" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 1 object (1 IFCAIRTOAIRHEATRECOVERY)
    Reference = "HRU 375 EV" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCAIRTOAIRHEATRECOVERY) | on 1 type object
    Manufacturer = "Itho Daalderop" (IFCLABEL)
  Constraints | properties | on 1 object (1 IFCAIRTOAIRHEATRECOVERY)
    Elevation from Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "None" (IFCTEXT)
    Offset from Host = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 type object
    Default Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCAIRTOAIRHEATRECOVERY)
    Area = 6.51060794502126 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.313298417471935 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 type object
    Depth = 430. (IFCLENGTHMEASURE) [MILLI METRE]
    Drain Diameter = 16. (IFCLENGTHMEASURE) [MILLI METRE]
    Exhaust Air Out Diameter = 160. (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 1248. (IFCLENGTHMEASURE) [MILLI METRE]
    Return Air In Diameter = 160. (IFCLENGTHMEASURE) [MILLI METRE]
    Supply Air In Diameter = 160. (IFCLENGTHMEASURE) [MILLI METRE]
    Supply Air Out Diameter = 160. (IFCLENGTHMEASURE) [MILLI METRE]
    Width = 600. (IFCLENGTHMEASURE) [MILLI METRE]
  Electrical | properties | on 1 object (1 IFCAIRTOAIRHEATRECOVERY)
    Power = 0. (IFCPOWERMEASURE) [WATT]
  Electrical | properties | on 1 type object
    Electrical Connection = "Earthed Plug" (IFCTEXT)
    Frequency = 50. (IFCFREQUENCYMEASURE) [HERTZ]
    Phase = 1 (IFCINTEGER)
    Voltage = 230. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
  Identity Data | properties | on 1 object (1 IFCAIRTOAIRHEATRECOVERY)
    Function Code = "" (IFCTEXT)
    Mark = "1" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Article Description = "WTW-unit 375 met elektrische voorverwarming, randaarde stekker, geschikt voor zonering" (IFCTEXT)
    Article Type = "HRU 375 EV" (IFCTEXT)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Base Family Version = "25.01" (IFCTEXT)
    CB-NL Class = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Content Supplier URL = "www.MEPcontent.com" (IFCTEXT)
    Copyright = "© Trimble Europe BV" (IFCTEXT)
    Custom = FALSE (IFCBOOLEAN)
    Description = "WTW-unit 375 met elektrische voorverwarming, randaarde stekker, geschikt voor zonering" (IFCTEXT)
    EMCS Version = "5.0" (IFCTEXT)
    ETIM Article Class = "EC011285" (IFCTEXT)
    Family Version = "24.11" (IFCTEXT)
    GLN = "8712922000014" (IFCTEXT)
    GTIN = "8713418053354" (IFCTEXT)
    Internal Art. No. = "" (IFCTEXT)
    MEPcontent Class = "AIR_HEATER_HEAT_RECOVERY" (IFCTEXT)
    Manufacturer = "Itho Daalderop" (IFCTEXT)
    Manufacturer Art. No. = "03-00854" (IFCTEXT)
    Manufacturer URL = "https://www.ithodaalderop.nl/nl-NL/consument/productoverzicht/A04_02" (IFCTEXT)
    Model = "HRU 375 EV" (IFCTEXT)
    OmniClass Number = "23.75.10.34.21" (IFCTEXT)
    OmniClass Title = "Heat Exchangers for Ventilation Air" (IFCTEXT)
    Product Line = "Itho Daalderop" (IFCTEXT)
    Revit Version = "2022" (IFCTEXT)
    Stabu Code = "" (IFCTEXT)
    Type Name = "HRU 375 EV" (IFCTEXT)
    URL = "https://mep.trimble.com" (IFCTEXT)
    Watermarked By = "https://mep.trimble.com" (IFCTEXT)
    Wholesaler = "" (IFCTEXT)
    Wholesaler Art. No. = "" (IFCTEXT)
  Mechanical | properties | on 1 object (1 IFCAIRTOAIRHEATRECOVERY)
    System Classification = "Supply Air,Exhaust Air,Supply Air,Return Air,Sanitary,Power" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Mechanical | properties | on 1 type object
    Classification = "None" (IFCIDENTIFIER)
  Mechanical - Flow | properties | on 1 object (1 IFCAIRTOAIRHEATRECOVERY)
    Drain Fixture Units = 0. (IFCREAL)
    Exhaust Air Out Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Return Air In Flow 1 = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Return Air In Flow 2 = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Supply Air In Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Supply Air Out Flow 1 = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Supply Air Out Flow 2 = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
  Phasing | properties | on 1 object (1 IFCAIRTOAIRHEATRECOVERY)
    Phase Created = "New Construction" (IFCLABEL)
  Visibility | properties | on 1 object (1 IFCAIRTOAIRHEATRECOVERY)
    Mounting Option = "Floor Mounted Vertical" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
    Reference = "Level 1" (IFCIDENTIFIER)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDING)
    AboveGround = UNKNOWN (IFCLOGICAL)
    Reference = "Project Information" (IFCIDENTIFIER)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
    Reference = "Project Information" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDING)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Project Information" (IFCIDENTIFIER)
  Pset_BuildingSystemCommon | properties | on 1 object (1 IFCBUILDING)
    Reference = "Project Information" (IFCIDENTIFIER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Materials and Finishes | properties | on 1 type object
    Black = "Color RGB 043-043-044" (IFCLABEL)
    Grey = "Color RGB 135-133-129" (IFCLABEL)
    White = "Color RGB 236-236-231" (IFCLABEL)