IFC building model
Schema: "IFC4"
Description: "ViewDefinition [CoordinationView_V2.0]"
Description: "RevitIdentifiers [VersionGUID: fbf85263-9754-4bc0-8e4d-a28fdc654d3a, NumberOfSaves: 0]"
Time stamp: "2025-07-22T10:10:19+02:00"
Preprocessor: "ODA SDAI 22.12"
Originating system: "Autodesk Revit 23.1.50.23 (ENU) - IFC 23.3.1.0"
Application: "Autodesk Revit 2023 (ENU)" version "2023" identifier "Revit" by Organization "Autodesk Revit 2023 (ENU)"

People and organizations
  Person "sergiu_pop" of Organization (no name given)
  Owner history of Person "sergiu_pop" of Organization (no name given) | application "Autodesk Revit 2023 (ENU)" version "2023" identifier "Revit" by Organization "Autodesk Revit 2023 (ENU)" | change NOCHANGE | created 1753168219 (2025-07-22T07:10:19Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  IONCONCENTRATIONUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  THERMALCONDUCTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  MASSFLOWRATEUNIT: derived
  ROTATIONALFREQUENCYUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  ENERGYUNIT: JOULE
  USERDEFINED: derived "Luminous Efficacy"
  USERDEFINED: derived "Electrical Resistivity"
  SOUNDPOWERUNIT: derived
  SOUNDPRESSUREUNIT: derived
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived
  SPECIFICHEATCAPACITYUNIT: derived
  HEATFLUXDENSITYUNIT: derived
  HEATINGVALUEUNIT: derived
  VAPORPERMEABILITYUNIT: derived
  DYNAMICVISCOSITYUNIT: derived
  THERMALEXPANSIONCOEFFICIENTUNIT: derived
  MODULUSOFELASTICITYUNIT: derived
  ISOTHERMALMOISTURECAPACITYUNIT: derived
  MOISTUREDIFFUSIVITYUNIT: derived
  AREADENSITYUNIT: derived
  MASSPERLENGTHUNIT: derived
  THERMALRESISTANCEUNIT: derived
  ACCELERATIONUNIT: derived
  ANGULARVELOCITYUNIT: derived
  LINEARSTIFFNESSUNIT: derived
  WARPINGCONSTANTUNIT: derived
  LINEARMOMENTUNIT: derived
  TORQUEUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "VE_Air Heater_Heat Recovery_MEPcontent_Itho Daalderop_HRU 400_NL-NL:HRU 400" | object type "VE_Air Heater_Heat Recovery_MEPcontent_Itho Daalderop_HRU 400_NL-NL:HRU 400" | names: "VE_Air Heater_Heat Recovery_MEPcontent_Itho Daalderop_HRU 400_NL-NL:HRU 400:24000" | material: constituents ("Color RAL 9003": "Color RAL 9003", "Color RGB 000-000-255": "Color RGB 000-000-255", "Color RGB 110-110-100": "Color RGB 110-110-100") | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators, Other, Constraints, Dimensions, Electrical - Loads

Types
  IFCBUILDINGELEMENTPROXYTYPE "VE_Air Heater_Heat Recovery_MEPcontent_Itho Daalderop_HRU 400_NL-NL:HRU 400" | 1 occurrence | material: constituents ("Equipment": "Color RAL 9003", "Color RGB 000-000-255": "Color RGB 000-000-255", "Equipment": "Color RGB 110-110-100") | property sets: Other, Constraints, Dimensions, Electrical, Identity Data, Materials and Finishes

Property sets
  Pset_SiteCommon | properties | on 1 object (1 IFCSITE)
    Reference = "Project Information" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "HRU 400" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDING)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Project Information" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
  Pset_EnvironmentalImpactIndicators | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "HRU 400" (IFCIDENTIFIER)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
    Reference = "Level 1" (IFCIDENTIFIER)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDING)
    AboveGround = UNKNOWN (IFCLOGICAL)
    Reference = "Project Information" (IFCIDENTIFIER)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
    Reference = "Project Information" (IFCIDENTIFIER)
  Pset_BuildingSystemCommon | properties | on 1 object (1 IFCBUILDING)
    Reference = "Project Information" (IFCIDENTIFIER)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level 1" (IFCLABEL)
    Type Id = "1899" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Back Clearance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Category = "Mechanical Equipment" (IFCLABEL)
    Condens Length Middle Safe = 346. (IFCLENGTHMEASURE) [MILLI METRE]
    Condens Length Side Safe = 140. (IFCLENGTHMEASURE) [MILLI METRE]
    Depth of Reference Line = 412. (IFCLENGTHMEASURE) [MILLI METRE]
    Drain Height = 107. (IFCLENGTHMEASURE) [MILLI METRE]
    Family = "VE_Air Heater_Heat Recovery_MEPcontent_Itho Daalderop_HRU 400_NL-NL" (IFCLABEL)
    Family and Type = "VE_Air Heater_Heat Recovery_MEPcontent_Itho Daalderop_HRU 400_NL-NL: HRU 400" (IFCLABEL)
    Front Clearance = 550. (IFCLENGTHMEASURE) [MILLI METRE]
    Height of Reference Line = 100. (IFCLENGTHMEASURE) [MILLI METRE]
    Left Clearance Safe = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    Leg Height Safe = 253. (IFCLENGTHMEASURE) [MILLI METRE]
    Legs Visibility = FALSE (IFCBOOLEAN)
    Offset from Right Side = 320. (IFCLENGTHMEASURE) [MILLI METRE]
    Reference Line Angle = 270. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference Line Length = 346. (IFCLENGTHMEASURE) [MILLI METRE]
    Right Cleareance Safe = 120. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Clearance Safe = 200. (IFCLENGTHMEASURE) [MILLI METRE]
    Type = "HRU 400" (IFCLABEL)
    Type Id = "23985" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Mechanical Equipment" (IFCLABEL)
    Family Name = "VE_Air Heater_Heat Recovery_MEPcontent_Itho Daalderop_HRU 400_NL-NL" (IFCTEXT)
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation from Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "None" (IFCTEXT)
    Offset from Host = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 type object
    Default Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 5.3161877318996664 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.36704580814464866 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 type object
    Depth = 580. (IFCLENGTHMEASURE) [MILLI METRE]
    Drain Diameter = 40. (IFCLENGTHMEASURE) [MILLI METRE]
    Exhaust Air Diameter = 180. (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 1064. (IFCLENGTHMEASURE) [MILLI METRE]
    Return Air Diameter = 180. (IFCLENGTHMEASURE) [MILLI METRE]
    Supply Air Anti-Freezing Diameter = 100. (IFCLENGTHMEASURE) [MILLI METRE]
    Supply Air Diameter = 180. (IFCLENGTHMEASURE) [MILLI METRE]
    Width = 640. (IFCLENGTHMEASURE) [MILLI METRE]
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Mark = "1" (IFCTEXT)
  Identity Data | properties | on 1 type object
    Article Description = "Warmteterugwinunit" (IFCTEXT)
    Article Type = "HRU 400" (IFCTEXT)
    Base Family Version = "25.09" (IFCTEXT)
    Content Supplier URL = "www.MEPcontent.com" (IFCTEXT)
    Copyright = "© Trimble Europe BV" (IFCTEXT)
    Custom = FALSE (IFCBOOLEAN)
    Description = "Warmteterugwinunit" (IFCTEXT)
    EMCS Version = "4.0" (IFCTEXT)
    ETIM Article Class = "EC011285" (IFCTEXT)
    Family Version = "12.08" (IFCTEXT)
    GLN = "8712922000014" (IFCTEXT)
    MEPcontent Class = "AIR_HEATER_HEAT_RECOVERY" (IFCTEXT)
    Manufacturer = "Itho Daalderop" (IFCTEXT)
    Manufacturer Art. No. = "M1-03763" (IFCTEXT)
    Manufacturer URL = "https://www.ithodaalderop.nl" (IFCTEXT)
    Model = "HRU 400" (IFCTEXT)
    OmniClass Number = "23.75.10.34.21" (IFCTEXT)
    OmniClass Title = "Heat Exchangers for Ventilation Air" (IFCTEXT)
    Product Line = "Itho Daalderop" (IFCTEXT)
    Revit Version = "2023" (IFCTEXT)
    Type Name = "HRU 400" (IFCTEXT)
    URL = "https://mep.trimble.com" (IFCTEXT)
    Watermarked By = "https://mep.trimble.com" (IFCTEXT)
  Electrical - Loads | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Power = 0. (IFCPOWERMEASURE) [WATT]
  Mechanical | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    System Classification = "Power,Return Air,Exhaust Air,Supply Air,Return Air,Supply Air,Sanitary" (IFCTEXT)
  Mechanical | properties | on 1 type object
    Air Flow Rate = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Classification = "None" (IFCIDENTIFIER)
    Heating Power = 0. (IFCPOWERMEASURE) [WATT]
    Nominal Flow Rate = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
  Mechanical - Flow | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Drain Fixture Units = 0. (IFCREAL)
    Exhaust Air Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Return Air from House Flow 2 = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Return Air from House Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Supply Air Anti-Freezing Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Supply Air Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Supply Air to House Flow 2 = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Supply Air to House Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
  Phasing | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Phase Created = "New Construction" (IFCLABEL)
  Visibility | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Condens Length Front-Back = 140. (IFCLENGTHMEASURE) [MILLI METRE]
    Condens Length Left-Right = 346. (IFCLENGTHMEASURE) [MILLI METRE]
    Condens Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Floor Mounted = FALSE (IFCBOOLEAN)
    Floor Mounted Legs = FALSE (IFCBOOLEAN)
    Left Side Condensate Drain = FALSE (IFCBOOLEAN)
    Left-Back Side Condensate Drain = FALSE (IFCBOOLEAN)
    Left-Front Side Condensate Drain = FALSE (IFCBOOLEAN)
    Leg Height = 253. (IFCLENGTHMEASURE) [MILLI METRE]
    Right Side Condensate Drain = TRUE (IFCBOOLEAN)
    Right-Back Side Condensate Drain = FALSE (IFCBOOLEAN)
    Right-Front Side Condensate Drain = FALSE (IFCBOOLEAN)
    Rotate Service Space = FALSE (IFCBOOLEAN)
    Rotate Unit = FALSE (IFCBOOLEAN)
    Show Service Space = FALSE (IFCBOOLEAN)
    Wall Mount = TRUE (IFCBOOLEAN)
  Visibility | properties | on 1 type object
    Condens Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Electrical | properties | on 1 type object
    Voltage = 229.99999964295171 (IFCELECTRICVOLTAGEMEASURE) [VOLT]
  Materials and Finishes | properties | on 1 type object
    Blue = "Color RGB 000-000-255" (IFCLABEL)
    Grey = "Color RGB 110-110-100" (IFCLABEL)
    Service Space = "Color RGB 218-227-224" (IFCLABEL)
    White = "Color RAL 9003" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 1 type object
    Manufacturer = "Itho Daalderop" (IFCLABEL)