IFC building model
Schema: "IFC4"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Project Number"
Time stamp: "2023-10-17T12:15:12"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "21.0.0.383 - Exporter 21.1.0.0 - Default UI"
Application: "Autodesk Revit 2021 (ENU)" version "2021" identifier "Revit" by Organization "Autodesk Revit 2021 (ENU)"

People and organizations
  Person "gheorghe_vizitiu" of Organization (no name given)
  Owner history of Person "gheorghe_vizitiu" of Organization (no name given) | application "Autodesk Revit 2021 (ENU)" version "2021" identifier "Revit" by Organization "Autodesk Revit 2021 (ENU)" | change NOCHANGE | created 1696480178 (2023-10-05T04:29:38Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 23′ 13.199999″ | longitude -71° 14′ 31.199999″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here"
      IFCBUILDINGSTOREY "F00" | long name "F00" | object type "Level:Floor Level" | elevation 0.
        contains 4 elements
          1 x IFCPUMP | type IFCPUMPTYPE "HC_Heat Pump_MEPcontent_Itho Daalderop_WPU 5G Module_NL-NL:THIS IS A TYPE CATALOG FAMILY" | object type "HC_Heat Pump_MEPcontent_Itho Daalderop_WPU 5G Module_NL-NL:THIS IS A TYPE CATALOG FAMILY" | names: "HC_Heat Pump_MEPcontent_Itho Daalderop_WPU 5G Module_NL-NL:THIS IS A TYPE CATALOG FAMILY:1316623" | material: constituents "MaterialConstituentSet" ("Color RGB 187-080-046": "Color RGB 187-080-046", "Color RGB 187-080-046": "Color RGB 187-080-046", "Color RGB 187-080-046": "Color RGB 187-080-046", "Color RGB 050-050-050": "Color RGB 050-050-050", "Color RGB 044-117-226": "Color RGB 044-117-226", "Color RGB 044-117-226": "Color RGB 044-117-226", "Color RGB 044-117-226": "Color RGB 044-117-226", "Color RGB 044-117-226": "Color RGB 044-117-226", "Color RGB 044-117-226": "Color RGB 044-117-226", "Color RGB 044-117-226": "Color RGB 044-117-226", "Color RGB 044-117-226": "Color RGB 044-117-226", "Color RGB 044-117-226": "Color RGB 044-117-226", "Color RGB 044-117-226": "Color RGB 044-117-226", "Color RGB 044-117-226": "Color RGB 044-117-226", "Color RGB 044-117-226": "Color RGB 044-117-226", "Color RGB 044-117-226": "Color RGB 044-117-226", "Color RGB 044-117-226": "Color RGB 044-117-226", "Color RGB 044-117-226": "Color RGB 044-117-226", "Color RGB 044-117-226": "Color RGB 044-117-226", "Color RGB 044-117-226": "Color RGB 044-117-226") | property sets: Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation, Pset_PumpTypeCommon, Constraints, Dimensions, Electrical - Loads
          1 x IFCPUMP | type IFCPUMPTYPE "HC_Heat Pump_MEPcontent_Itho Daalderop_WPV 5_Top Cover_NL-NL-Shared:Top Cover" | object type "HC_Heat Pump_MEPcontent_Itho Daalderop_WPV 5_Top Cover_NL-NL-Shared:Top Cover" | names: "HC_Heat Pump_MEPcontent_Itho Daalderop_WPV 5_Top Cover_NL-NL-Shared:Top Cover:1316758" | material: "Color RGB 050-050-050" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation, Pset_PumpTypeCommon, Constraints, Dimensions, Electrical - Loads
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "HC_Heat Pump_Itho Daalderop_WPU 5G_Onderomkasting 3G_Shared:WPU 5G - Onderomkasting 3G" | object type "HC_Heat Pump_Itho Daalderop_WPU 5G_Onderomkasting 3G_Shared:WPU 5G - Onderomkasting 3G" | names: "HC_Heat Pump_Itho Daalderop_WPU 5G_Onderomkasting 3G_Shared:WPU 5G - Onderomkasting 3G:1316847" | material: constituents "MaterialConstituentSet" ("Color RGB 050-050-050": "Color RGB 050-050-050", "Color RGB 050-050-050": "Color RGB 050-050-050", "Color RAL 9003": "Color RAL 9003", "Color RGB 050-050-050": "Color RGB 050-050-050", "Color RGB 050-050-050": "Color RGB 050-050-050", "Color RGB 050-050-050": "Color RGB 050-050-050", "Color RGB 050-050-050": "Color RGB 050-050-050", "Color RAL 9006": "Color RAL 9006", "Color RAL 9006": "Color RAL 9006", "Color RAL 9006": "Color RAL 9006", "Color RAL 9006": "Color RAL 9006", "Color RAL 9006": "Color RAL 9006", "Color RAL 9006": "Color RAL 9006", "Color RAL 9006": "Color RAL 9006", "Color RAL 9006": "Color RAL 9006", "Color RAL 9006": "Color RAL 9006", "Color RAL 9006": "Color RAL 9006", "Color RAL 9006": "Color RAL 9006", "Color RAL 9006": "Color RAL 9006", "Color RAL 9006": "Color RAL 9006") | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation, Constraints, Dimensions, Identity Data
          1 x IFCPUMP | type IFCPUMPTYPE "HC_Heat Pump_MEPcontent_Itho Daalderop_WPV-H 3G_NL-NL:WPV-H 200L 3G" | object type "HC_Heat Pump_MEPcontent_Itho Daalderop_WPV-H 3G_NL-NL:WPV-H 200L 3G" | names: "HC_Heat Pump_MEPcontent_Itho Daalderop_WPV-H 3G_NL-NL:WPV-H 200L 3G:1357293" | material: constituents "MaterialConstituentSet" ("Color RAL 9006": "Color RAL 9006", "Color RAL 9006": "Color RAL 9006", "Color RAL 9006": "Color RAL 9006", "Color RAL 9006": "Color RAL 9006", "Color RAL 9006": "Color RAL 9006", "Color RAL 9006": "Color RAL 9006", "Color RAL 9006": "Color RAL 9006", "Color RAL 9006": "Color RAL 9006", "Color RAL 9006": "Color RAL 9006", "Color RAL 9006": "Color RAL 9006", "Color RAL 9006": "Color RAL 9006", "Color RAL 9006": "Color RAL 9006", "Color RAL 9006": "Color RAL 9006", "Color RAL 9006": "Color RAL 9006", "Color RAL 9006": "Color RAL 9006", "Color RAL 9006": "Color RAL 9006", "Color RAL 9006": "Color RAL 9006", "Color RAL 9006": "Color RAL 9006", "Color RAL 9006": "Color RAL 9006", "Color RAL 9006": "Color RAL 9006") | property sets: Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation, Pset_PumpTypeCommon, Constraints, Dimensions, Electrical - Loads

Types
  IFCPUMPTYPE "HC_Heat Pump_MEPcontent_Itho Daalderop_WPU 5G Module_NL-NL:THIS IS A TYPE CATALOG FAMILY" | 1 occurrence | material: constituents "MaterialConstituentSet" ("Color RAL 9003": "Color RAL 9003", "Color RGB 255-000-000": "Color RGB 255-000-000", "Color RGB 187-080-046": "Color RGB 187-080-046", "Color RGB 044-117-226": "Color RGB 044-117-226", "Color RGB 000-000-255": "Color RGB 000-000-255", "Color RAL 9006": "Color RAL 9006", "Color RGB 050-050-050": "Color RGB 050-050-050") | property sets: Constraints, Dimensions, Electrical, Electrical - Loads, Identity Data, Materials and Finishes
  IFCPUMPTYPE "HC_Heat Pump_MEPcontent_Itho Daalderop_WPV 5_Top Cover_NL-NL-Shared:Top Cover" | 1 occurrence | material: "Color RGB 050-050-050" | property sets: Constraints, Dimensions, Electrical - Loads, Identity Data, Materials and Finishes, Mechanical
  IFCBUILDINGELEMENTPROXYTYPE "HC_Heat Pump_Itho Daalderop_WPU 5G_Onderomkasting 3G_Shared:WPU 5G - Onderomkasting 3G" | 1 occurrence | material: constituents "MaterialConstituentSet" ("Color RAL 9003": "Color RAL 9003", "Color RGB 050-050-050": "Color RGB 050-050-050", "Color RGB 236-236-231": "Color RGB 236-236-231", "Color RAL 9006": "Color RAL 9006", "Color RGB 044-117-226": "Color RGB 044-117-226") | property sets: Constraints, Identity Data, Materials and Finishes, Mechanical, Other, Pset_BuildingElementProxyCommon
  IFCPUMPTYPE "HC_Heat Pump_MEPcontent_Itho Daalderop_WPV-H 3G_NL-NL:WPV-H 200L 3G" | 1 occurrence | material: constituents "MaterialConstituentSet" ("Color RGB 050-050-050": "Color RGB 050-050-050", "Color RAL 9003": "Color RAL 9003", "Color RAL 9006": "Color RAL 9006") | property sets: Constraints, Dimensions, Electrical, Identity Data, Materials and Finishes, Mechanical

Property sets
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Floor Level" (IFCTEXT)
  Pset_SiteCommon | properties | on 1 object (1 IFCSITE)
    Reference = "Project Information" (IFCIDENTIFIER)
  Dimensions | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    S4R_Use_nominal_diameter = TRUE (IFCBOOLEAN)
  Dimensions | properties | on 1 object (1 IFCPUMP)
    Area = 6.57538493058046 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.134498750108364 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    a = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Dimensions | properties | on 1 object (1 IFCPUMP)
    Area = 0.41288343541734 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.0161845391422783 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 1.92525091254859 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.0373062976606706 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCPUMP)
    Area = 4.99664314600458 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.463913280447809 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 type object
    Depth = 600. (IFCLENGTHMEASURE) [MILLI METRE]
    Domestic Cold Water Diameter = 25.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Domestic Hot Water Diameter = 25.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 830. (IFCLENGTHMEASURE) [MILLI METRE]
    Hydronic Return 1 Diameter = 25.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Hydronic Return 2 Diameter = 25.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Hydronic Supply 1 Diameter = 25.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Hydronic Supply 2 Diameter = 25.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Module Foundationplate Depth = 389. (IFCLENGTHMEASURE) [MILLI METRE]
    Module Foundationplate Width = 560. (IFCLENGTHMEASURE) [MILLI METRE]
    Module Height = 611.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Use Nominal Diameter = TRUE (IFCBOOLEAN)
    Width = 600. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 type object
    Depth = 600. (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 31. (IFCLENGTHMEASURE) [MILLI METRE]
    Width = 600. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions: 1 more content on 0 objects not shown
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCPUMP)
    Casing Manufacturer Art. No. = "04-00073" (IFCTEXT)
    Function Code = "" (IFCTEXT)
    Mark = "4" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCPUMP)
    Function Code = "" (IFCTEXT)
    Mark = "7" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Function Code = "" (IFCTEXT)
    Mark = "9" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCPUMP)
    Function Code = "" (IFCTEXT)
    Mark = "10" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "F00" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Article Description = "" (IFCTEXT)
    Article Type = "" (IFCTEXT)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Base Family Version = "23.10" (IFCTEXT)
    CB-NL Class = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Content Supplier URL = "www.MEPcontent.com" (IFCTEXT)
    Copyright = "© Trimble Europe BV" (IFCTEXT)
    Custom = FALSE (IFCBOOLEAN)
    Description = "" (IFCTEXT)
    EMCS Version = "5.0" (IFCTEXT)
    ETIM Article Class = "EC011794" (IFCTEXT)
    Family Version = "11.25" (IFCTEXT)
    GLN = "" (IFCTEXT)
    GTIN = "" (IFCTEXT)
    Internal Art. No. = "" (IFCTEXT)
    MEPcontent Class = "HEATPUMP" (IFCTEXT)
    Manufacturer = "Itho Daalderop" (IFCTEXT)
    Manufacturer Art. No. = "" (IFCTEXT)
    Manufacturer URL = "" (IFCTEXT)
    Model = "" (IFCTEXT)
    OmniClass Number = "23.75.10.21" (IFCTEXT)
    OmniClass Title = "Heat Pumps" (IFCTEXT)
    Product Line = "Itho Daalderop" (IFCTEXT)
    Revit Version = "2021" (IFCTEXT)
    Stabu Code = "" (IFCTEXT)
    Type Name = "THIS IS A TYPE CATALOG FAMILY" (IFCTEXT)
    URL = "https://mep.trimble.com" (IFCTEXT)
    Watermarked By = "https://mep.trimble.com" (IFCTEXT)
    Wholesaler = "" (IFCTEXT)
    Wholesaler Art. No. = "" (IFCTEXT)
  Identity Data | properties | on 1 type object
    Article Description = "Top cover for heat pump" (IFCTEXT)
    Article Type = "Top Cover" (IFCTEXT)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Base Family Version = "23.10" (IFCTEXT)
    CB-NL Class = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Content Supplier URL = "www.MEPcontent.com" (IFCTEXT)
    Copyright = "© Trimble Europe BV" (IFCTEXT)
    Custom = FALSE (IFCBOOLEAN)
    Description = "Top cover for heat pump" (IFCTEXT)
    EMCS Version = "5.0" (IFCTEXT)
    ETIM Article Class = "EC012266" (IFCTEXT)
    Family Version = "22.12" (IFCTEXT)
    GLN = "8712922000014" (IFCTEXT)
    GTIN = "8713418041702" (IFCTEXT)
    Internal Art. No. = "" (IFCTEXT)
    MEPcontent Class = "HEATPUMP" (IFCTEXT)
    Manufacturer = "Itho Daalderop" (IFCTEXT)
    Manufacturer Art. No. = "04-00092" (IFCTEXT)
    Manufacturer URL = "https://zakelijk.ithodaalderop.nl/ean/08713418041702" (IFCTEXT)
    Model = "Top Cover" (IFCTEXT)
    OmniClass Number = "23.75.10.17.17" (IFCTEXT)
    OmniClass Title = "Combined Heating/Cooking Units" (IFCTEXT)
    Product Line = "Itho Daalderop" (IFCTEXT)
    Revit Version = "2021" (IFCTEXT)
    Stabu Code = "" (IFCTEXT)
    Type Name = "Top Cover" (IFCTEXT)
    URL = "https://mep.trimble.com" (IFCTEXT)
    Watermarked By = "https://mep.trimble.com" (IFCTEXT)
    Wholesaler = "" (IFCTEXT)
    Wholesaler Art. No. = "" (IFCTEXT)
  Identity Data: 2 more contents on 0 objects not shown
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Client Name" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Project Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "Project Number" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other | properties | on 1 object (1 IFCPUMP)
    Back Clearance Safe = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Category = "Mechanical Equipment" (IFCLABEL)
    Connection Set Hydronic + Expansion Vessel Safe = FALSE (IFCBOOLEAN)
    Connection Set Hydronic Safe = FALSE (IFCBOOLEAN)
    Connection Set Tap Water + Expansion Vessel Safe = FALSE (IFCBOOLEAN)
    Connection Set Tap Water Safe = FALSE (IFCBOOLEAN)
    Domestic Cold Water Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Domestic Cold Water Connection Depth = 265.7 (IFCLENGTHMEASURE) [MILLI METRE]
    Domestic Cold Water Connection Height = 794. (IFCLENGTHMEASURE) [MILLI METRE]
    Domestic Cold Water Connection Width = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Domestic Hot Water Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Domestic Hot Water Connection Depth = 205.7 (IFCLENGTHMEASURE) [MILLI METRE]
    Domestic Hot Water Connection Height = 794. (IFCLENGTHMEASURE) [MILLI METRE]
    Domestic Hot Water Connection Width = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Family = "HC_Heat Pump_MEPcontent_Itho Daalderop_WPU 5G Module_NL-NL: THIS IS A TYPE CATALOG FAMILY" (IFCLABEL)
    Family and Type = "HC_Heat Pump_MEPcontent_Itho Daalderop_WPU 5G Module_NL-NL: THIS IS A TYPE CATALOG FAMILY" (IFCLABEL)
    Front Clearance Safe = 500. (IFCLENGTHMEASURE) [MILLI METRE]
    Hydronic Return 1 Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Hydronic Return 1 Connection Depth = 354. (IFCLENGTHMEASURE) [MILLI METRE]
    Hydronic Return 1 Connection Height = 747.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Hydronic Return 1 Connection Width = 300. (IFCLENGTHMEASURE) [MILLI METRE]
    Hydronic Return 2 Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Hydronic Return 2 Connection Depth = 294. (IFCLENGTHMEASURE) [MILLI METRE]
    Hydronic Return 2 Connection Height = 747.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Hydronic Return 2 Connection Width = 300. (IFCLENGTHMEASURE) [MILLI METRE]
    Hydronic Supply 1 Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Hydronic Supply 1 Connection Depth = 234. (IFCLENGTHMEASURE) [MILLI METRE]
    Hydronic Supply 1 Connection Height = 747.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Hydronic Supply 1 Connection Width = 300. (IFCLENGTHMEASURE) [MILLI METRE]
    Hydronic Supply 2 Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Hydronic Supply 2 Connection Depth = 174. (IFCLENGTHMEASURE) [MILLI METRE]
    Hydronic Supply 2 Connection Height = 747.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Hydronic Supply 2 Connection Width = 300. (IFCLENGTHMEASURE) [MILLI METRE]
    Left Clearance Safe = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    Offset = 178. (IFCLENGTHMEASURE) [MILLI METRE]
    Right Clearance Safe = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    Right Domestic Cold Water Connection Safe = TRUE (IFCBOOLEAN)
    Right Domestic Hot Water Connection Safe = TRUE (IFCBOOLEAN)
    Right Hydronic Return Connection 1 Safe = TRUE (IFCBOOLEAN)
    Right Hydronic Return Connection 2 Safe = TRUE (IFCBOOLEAN)
    Right Hydronic Supply Connection 1 Safe = TRUE (IFCBOOLEAN)
    Right Hydronic Supply Connection 2 Safe = TRUE (IFCBOOLEAN)
    Show Casing-Base cabinet Safe = TRUE (IFCBOOLEAN)
    Show Casing-Frame and front panel Safe = FALSE (IFCBOOLEAN)
    Show Logo = FALSE (IFCBOOLEAN)
    Show Storage Tank = FALSE (IFCBOOLEAN)
    Storage Tank Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Storage Tank Position = 31. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Clearance Safe 2 = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Clearance Safe = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Cover Visibility = TRUE (IFCBOOLEAN)
    Total Depth = 615. (IFCLENGTHMEASURE) [MILLI METRE]
    Total Height = 830. (IFCLENGTHMEASURE) [MILLI METRE]
    Total Width = 600. (IFCLENGTHMEASURE) [MILLI METRE]
    Type = "HC_Heat Pump_MEPcontent_Itho Daalderop_WPU 5G Module_NL-NL: THIS IS A TYPE CATALOG FAMILY" (IFCLABEL)
    Type Id = "HC_Heat Pump_MEPcontent_Itho Daalderop_WPU 5G Module_NL-NL: THIS IS A TYPE CATALOG FAMILY" (IFCLABEL)
    Wall Offset Safe 2 = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    Wall Offset Safe = 15. (IFCLENGTHMEASURE) [MILLI METRE]
  Other | properties | on 1 object (1 IFCPUMP)
    Category = "Mechanical Equipment" (IFCLABEL)
    Family = "HC_Heat Pump_MEPcontent_Itho Daalderop_WPV 5_Top Cover_NL-NL-Shared: Top Cover" (IFCLABEL)
    Family and Type = "HC_Heat Pump_MEPcontent_Itho Daalderop_WPV 5_Top Cover_NL-NL-Shared: Top Cover" (IFCLABEL)
    Top Cover Visibility = TRUE (IFCBOOLEAN)
    Type = "HC_Heat Pump_MEPcontent_Itho Daalderop_WPV 5_Top Cover_NL-NL-Shared: Top Cover" (IFCLABEL)
    Type Id = "HC_Heat Pump_MEPcontent_Itho Daalderop_WPV 5_Top Cover_NL-NL-Shared: Top Cover" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Category = "Mechanical Equipment" (IFCLABEL)
    Family = "HC_Heat Pump_Itho Daalderop_WPU 5G_Onderomkasting 3G_Shared: WPU 5G - Onderomkasting 3G" (IFCLABEL)
    Family and Type = "HC_Heat Pump_Itho Daalderop_WPU 5G_Onderomkasting 3G_Shared: WPU 5G - Onderomkasting 3G" (IFCLABEL)
    Type = "HC_Heat Pump_Itho Daalderop_WPU 5G_Onderomkasting 3G_Shared: WPU 5G - Onderomkasting 3G" (IFCLABEL)
    Type Id = "HC_Heat Pump_Itho Daalderop_WPU 5G_Onderomkasting 3G_Shared: WPU 5G - Onderomkasting 3G" (IFCLABEL)
  Other | properties | on 1 object (1 IFCPUMP)
    Back Clearance Safe = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    Category = "Mechanical Equipment" (IFCLABEL)
    Family = "HC_Heat Pump_MEPcontent_Itho Daalderop_WPV-H 3G_NL-NL: WPV-H 200L 3G" (IFCLABEL)
    Family and Type = "HC_Heat Pump_MEPcontent_Itho Daalderop_WPV-H 3G_NL-NL: WPV-H 200L 3G" (IFCLABEL)
    Front Clearance Safe = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    Left Clearance Safe = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    Right Clearance Safe = 200. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Clearance Safe = 150. (IFCLENGTHMEASURE) [MILLI METRE]
    Type = "HC_Heat Pump_MEPcontent_Itho Daalderop_WPV-H 3G_NL-NL: WPV-H 200L 3G" (IFCLABEL)
    Type Id = "HC_Heat Pump_MEPcontent_Itho Daalderop_WPV-H 3G_NL-NL: WPV-H 200L 3G" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: Floor Level" (IFCLABEL)
    Family and Type = "Level: Floor Level" (IFCLABEL)
    Type = "Level: Floor Level" (IFCLABEL)
    Type Id = "Level: Floor Level" (IFCLABEL)
  Other | properties | on 1 type object
    Bottom Clearance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Category = "Mechanical Equipment" (IFCLABEL)
    Family Name = "HC_Heat Pump_MEPcontent_Itho Daalderop_WPU 5G Module_NL-NL" (IFCTEXT)
    Storage Tank Safe 2 = "HC_Heat Pump_MEPcontent_Itho Daalderop_WPV 5_Storage Tank_NL-NL-Shared: WPV 200L 3G" (IFCLABEL)
    Storage Tank Safe = "HC_Heat Pump_MEPcontent_Itho Daalderop_WPV 5_Storage Tank_NL-NL-Shared: WPV 150L 3G" (IFCLABEL)
    Top Cover = "HC_Heat Pump_MEPcontent_Itho Daalderop_WPV 5_Top Cover_NL-NL-Shared: Top Cover" (IFCLABEL)
    Type E (Elektrisch) = FALSE (IFCBOOLEAN)
    Type I (Individuele bron) = FALSE (IFCBOOLEAN)
  Other | properties | on 1 type object
    Category = "Mechanical Equipment" (IFCLABEL)
    Family Name = "HC_Heat Pump_MEPcontent_Itho Daalderop_WPV 5_Top Cover_NL-NL-Shared" (IFCTEXT)
  Other: 2 more contents on 0 objects not shown
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "GE_tag_level_floor_MEPcontent: standard" (IFCLABEL)
    Symbol at End 1 Default = TRUE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Pset_EnvironmentalImpactIndicators | properties | on 1 object (1 IFCPUMP) | on 1 type object
    Reference = "THIS IS A TYPE CATALOG FAMILY" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 1 object (1 IFCPUMP) | on 1 type object
    Reference = "Top Cover" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "WPU 5G - Onderomkasting 3G" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 1 object (1 IFCPUMP) | on 1 type object
    Reference = "WPV-H 200L 3G" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 4 objects (3 IFCPUMP, 1 IFCBUILDINGELEMENTPROXY) | on 4 type objects
    Manufacturer = "Itho Daalderop" (IFCLABEL)
  Pset_PumpTypeCommon | properties | on 1 object (1 IFCPUMP) | on 1 type object
    Reference = "THIS IS A TYPE CATALOG FAMILY" (IFCIDENTIFIER)
  Pset_PumpTypeCommon | properties | on 1 object (1 IFCPUMP) | on 1 type object
    Reference = "Top Cover" (IFCIDENTIFIER)
  Pset_PumpTypeCommon | properties | on 1 object (1 IFCPUMP) | on 1 type object
    Reference = "WPV-H 200L 3G" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCPUMP)
    Elevation from Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Level : F00" (IFCTEXT)
    Level = "Level: F00" (IFCLABEL)
    Offset from Host = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCPUMP)
    Elevation from Level = 829.999999999997 (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Level : F00" (IFCTEXT)
    Level = "Level: F00" (IFCLABEL)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset from Host = 829.999999999997 (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation from Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Level : F00" (IFCTEXT)
    Level = "Level: F00" (IFCLABEL)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset from Host = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCPUMP)
    Elevation from Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "None" (IFCTEXT)
    Offset from Host = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 4 type objects
    Default Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Electrical - Loads | properties | on 2 objects (2 IFCPUMP)
    Power = 0. (IFCPOWERMEASURE) [WATT]
  Electrical - Loads | properties | on 1 object (1 IFCPUMP)
    Circuit Number = "" (IFCTEXT)
    Panel = "" (IFCTEXT)
    Power = 0. (IFCPOWERMEASURE) [WATT]
  Electrical - Loads | properties | on 1 type object
    Voltage = 230. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
  Electrical - Loads | properties | on 1 type object
    Voltage = 229.999999642952 (IFCELECTRICVOLTAGEMEASURE) [VOLT]
  Mechanical | properties | on 1 object (1 IFCPUMP)
    System Classification = "Hydronic Supply,Domestic Hot Water,Power,Hydronic Return,Domestic Cold Water" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Mechanical | properties | on 1 object (1 IFCPUMP)
    System Classification = "Domestic Hot Water,Domestic Cold Water,Hydronic Return,Hydronic Supply,Power" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Mechanical | properties | on 2 type objects
    Classification = "Pump" (IFCIDENTIFIER)
  Mechanical | properties | on 2 type objects
    Classification = "None" (IFCIDENTIFIER)
  Mechanical - Flow | properties | on 1 object (1 IFCPUMP)
    Domestic Cold Water Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Domestic Hot Water Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Hydronic Return Flow 1 = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Hydronic Return Flow 2 = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Hydronic Supply Flow 1 = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Hydronic Supply Flow 2 = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
  Mechanical - Flow | properties | on 1 object (1 IFCPUMP)
    Domestic Cold Water Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Domestic Hot Water Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Hydronic Return Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Hydronic Supply Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
  Phasing | properties | on 3 objects (2 IFCPUMP, 1 IFCBUILDINGELEMENTPROXY)
    Phase Created = "3. New Construction" (IFCLABEL)
  Phasing | properties | on 1 object (1 IFCPUMP)
    Phase Created = "4. Plan over 10 years" (IFCLABEL)
  Visibility | properties | on 1 object (1 IFCPUMP)
    Connection Set Hydronic + Expansion Vessel = FALSE (IFCBOOLEAN)
    Connection Set Hydronic = FALSE (IFCBOOLEAN)
    Connection Set Tap Water + Expansion Vessel = FALSE (IFCBOOLEAN)
    Connection Set Tap Water = FALSE (IFCBOOLEAN)
    Front Clearance = 500. (IFCLENGTHMEASURE) [MILLI METRE]
    Left Clearance = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    Left Domestic Cold Water Connection = FALSE (IFCBOOLEAN)
    Left Domestic Hot Water Connection = FALSE (IFCBOOLEAN)
    Left Hydronic Return Connection 1 = FALSE (IFCBOOLEAN)
    Left Hydronic Return Connection 2 = FALSE (IFCBOOLEAN)
    Left Hydronic Supply Connection 1 = FALSE (IFCBOOLEAN)
    Left Hydronic Supply Connection 2 = FALSE (IFCBOOLEAN)
    Right Clearance = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    Right Domestic Cold Water Connection = TRUE (IFCBOOLEAN)
    Right Domestic Hot Water Connection = TRUE (IFCBOOLEAN)
    Right Hydronic Return Connection 1 = TRUE (IFCBOOLEAN)
    Right Hydronic Return Connection 2 = TRUE (IFCBOOLEAN)
    Right Hydronic Supply Connection 1 = TRUE (IFCBOOLEAN)
    Right Hydronic Supply Connection 2 = TRUE (IFCBOOLEAN)
    Show Casing = TRUE (IFCBOOLEAN)
    Show Service Space = FALSE (IFCBOOLEAN)
    Show frame and front panel = FALSE (IFCBOOLEAN)
    Standard Connection = FALSE (IFCBOOLEAN)
    Storage Tank = "HC_Heat Pump_MEPcontent_Itho Daalderop_WPV 5_Top Cover_NL-NL-Shared: Top Cover" (IFCLABEL)
    Top Clearance = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    Wall Offset = 15. (IFCLENGTHMEASURE) [MILLI METRE]
  Visibility | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Show Casing = TRUE (IFCBOOLEAN)
  Visibility | properties | on 1 object (1 IFCPUMP)
    Back Clearance = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    Front Clearance = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    Left Clearance = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    Right Clearance = 200. (IFCLENGTHMEASURE) [MILLI METRE]
    Show Service Space = FALSE (IFCBOOLEAN)
    Top Clearance = 150. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "WPU 5G - Onderomkasting 3G" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDING)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Project Information" (IFCIDENTIFIER)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
    Reference = "Floor Level" (IFCIDENTIFIER)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDING)
    AboveGround = UNKNOWN (IFCLOGICAL)
    Reference = "Project Information" (IFCIDENTIFIER)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
    Reference = "Project Information" (IFCIDENTIFIER)
  Pset_BuildingSystemCommon | properties | on 1 object (1 IFCBUILDING)
    Reference = "Project Information" (IFCIDENTIFIER)
  Electrical | properties | on 1 type object
    Hertz = 50. (IFCFREQUENCYMEASURE) [HERTZ]
    Phase = 1 (IFCINTEGER)
  Electrical | properties | on 1 type object
    Hertz = 50. (IFCFREQUENCYMEASURE) [HERTZ]
    Phase = 1 (IFCINTEGER)
    Voltage = 229.999999642952 (IFCELECTRICVOLTAGEMEASURE) [VOLT]
  Materials and Finishes | properties | on 1 type object
    Black = "Color RGB 050-050-050" (IFCLABEL)
    Blue = "Color RGB 000-000-255" (IFCLABEL)
    Connection = "Color RGB 187-080-046" (IFCLABEL)
    Light Blue = "Color RGB 044-117-226" (IFCLABEL)
    Light Grey = "Color RAL 9006" (IFCLABEL)
    Red = "Color RGB 255-000-000" (IFCLABEL)
    White = "Color RAL 9003" (IFCLABEL)
  Materials and Finishes | properties | on 1 type object
    Black = "Color RGB 050-050-050" (IFCLABEL)
  Materials and Finishes | properties | on 1 type object
    Black = "Color RGB 050-050-050" (IFCLABEL)
    Blue = "Color RGB 044-117-226" (IFCLABEL)
    Grey = "Color RGB 236-236-231" (IFCLABEL)
    Light Grey = "Color RAL 9006" (IFCLABEL)
    White = "Color RAL 9003" (IFCLABEL)
  Materials and Finishes | properties | on 1 type object
    Black = "Color RGB 050-050-050" (IFCLABEL)
    Light Grey = "Color RAL 9006" (IFCLABEL)
    White = "Color RAL 9003" (IFCLABEL)
  Mechanical - Loads | properties | on 1 type object
    Cooling Power = 0. (IFCPOWERMEASURE) [WATT]
    Heating Power = 25000. (IFCPOWERMEASURE) [WATT]
    Operation Point Cooling = "" (IFCTEXT)
    Operation Point Heating = "" (IFCTEXT)