,z_Sheet steel door with ventilation slots and plastic insert semi-transparent##OTHER##,z_Sheet steel door with ventilation slots##OTHER##,z_Sheet steel door##OTHER##,z_Normal Frame##OTHER##,z_Door_on_Right_Visibility##OTHER##,Width##LENGTH##MILLIMETERS,Weight - Mass##MASS##KILOGRAMS,Type Comments##OTHER##,Space units [SU]##OTHER##,Shock resistance level##OTHER##,Protection class##OTHER##,Panel width (PW)##OTHER##,Order code##OTHER##,Internal configuration option##OTHER##,Height##LENGTH##MILLIMETERS,Gird units (GU)##OTHER##,Enclosures and doors##OTHER##,Dissipated Power at Overtemperature ∆t 20K##ELECTRICAL_WATTAGE##WATTS,Description##OTHER##,Delivery types##OTHER##,Degree of protection##OTHER##,Accessories##OTHER##
CU14V,0,0,1,1,1,365,10,"ComfortLine Compact CU distribution boards for flush and hollow wall mounting*

with distribution panels, frames and sheet steel doors.",48,IK09,"II, insulated

I, grounded in connection with earthing set (accessories)",1,2CPX052607R9999,"DIN rail spacing 125 mm/150 mm

Fields for DIN rail devices with DIN rails of 35 x 7,5 mm and N/PE Quick-terminals (1 x ZK224 per field width)

Fields with mounting plates

Fields for terminal blocks with DIN rails of 35 x 7,5 mm insulated mounted (without N/PE Quick-terminals)",715,4,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",22.1,CU14V      Compact Distr.B 1PW 4R IP31,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Cable entry covers

Lock replacement parts

Sheet steel- and transparent doors

Media panels

Distribution panels

CombiLine modules"
CU15V,0,0,1,1,1,365,11.5,"ComfortLine Compact CU distribution boards for flush and hollow wall mounting*

with distribution panels, frames and sheet steel doors.",60,IK09,"II, insulated

I, grounded in connection with earthing set (accessories)",1,2CPX052608R9999,"DIN rail spacing 125 mm/150 mm

Fields for DIN rail devices with DIN rails of 35 x 7,5 mm and N/PE Quick-terminals (1 x ZK224 per field width)

Fields with mounting plates

Fields for terminal blocks with DIN rails of 35 x 7,5 mm insulated mounted (without N/PE Quick-terminals)",865,5,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",26.5,CU15V      Compact Distr.B 1PW 5R IP31,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Cable entry covers

Lock replacement parts

Sheet steel- and transparent doors

Media panels

Distribution panels

CombiLine modules"
CU16V,0,0,1,1,1,365,13.5,"ComfortLine Compact CU distribution boards for flush and hollow wall mounting*

with distribution panels, frames and sheet steel doors.",72,IK09,"II, insulated

I, grounded in connection with earthing set (accessories)",1,2CPX052609R9999,"DIN rail spacing 125 mm/150 mm

Fields for DIN rail devices with DIN rails of 35 x 7,5 mm and N/PE Quick-terminals (1 x ZK224 per field width)

Fields with mounting plates

Fields for terminal blocks with DIN rails of 35 x 7,5 mm insulated mounted (without N/PE Quick-terminals)",1015,6,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",30.9,CU16V      Compact Distr.B 1PW 6R IP31,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Cable entry covers

Lock replacement parts

Sheet steel- and transparent doors

Media panels

Distribution panels

CombiLine modules"
CU17V,0,0,1,1,1,365,16,"ComfortLine Compact CU distribution boards for flush and hollow wall mounting*

with distribution panels, frames and sheet steel doors.",84,IK09,"II, insulated

I, grounded in connection with earthing set (accessories)",1,2CPX052610R9999,"DIN rail spacing 125 mm/150 mm

Fields for DIN rail devices with DIN rails of 35 x 7,5 mm and N/PE Quick-terminals (1 x ZK224 per field width)

Fields with mounting plates

Fields for terminal blocks with DIN rails of 35 x 7,5 mm insulated mounted (without N/PE Quick-terminals)",1165,7,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",35.5,CU17V      Compact Distr.B 1PW 7R IP31,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Cable entry covers

Lock replacement parts

Sheet steel- and transparent doors

Media panels

Distribution panels

CombiLine modules"
CU18V,0,0,1,1,1,365,17.5,"ComfortLine Compact CU distribution boards for flush and hollow wall mounting*

with distribution panels, frames and sheet steel doors.",96,IK09,"II, insulated

I, grounded in connection with earthing set (accessories)",1,2CPX052611R9999,"DIN rail spacing 125 mm/150 mm

Fields for DIN rail devices with DIN rails of 35 x 7,5 mm and N/PE Quick-terminals (1 x ZK224 per field width)

Fields with mounting plates

Fields for terminal blocks with DIN rails of 35 x 7,5 mm insulated mounted (without N/PE Quick-terminals)",1315,8,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",39.9,CU18V      Compact Distr.B 1PW 8R IP31,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Cable entry covers

Lock replacement parts

Sheet steel- and transparent doors

Media panels

Distribution panels

CombiLine modules"
CU23V,0,0,1,1,1,615,12,"ComfortLine Compact CU distribution boards for flush and hollow wall mounting*

with distribution panels, frames and sheet steel doors.",72,IK09,"II, insulated

I, grounded in connection with earthing set (accessories)",2,2CPX052612R9999,"DIN rail spacing 125 mm/150 mm

Fields for DIN rail devices with DIN rails of 35 x 7,5 mm and N/PE Quick-terminals (1 x ZK224 per field width)

Fields with mounting plates

Fields for terminal blocks with DIN rails of 35 x 7,5 mm insulated mounted (without N/PE Quick-terminals)",565,3,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",35.1,CU23V      Compact Distr.B 2PW 3R IP31,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Cable entry covers

Lock replacement parts

Sheet steel- and transparent doors

Media panels

Distribution panels

CombiLine modules"
CU24V,0,0,1,1,1,615,15,"ComfortLine Compact CU distribution boards for flush and hollow wall mounting*

with distribution panels, frames and sheet steel doors.",96,IK09,"II, insulated

I, grounded in connection with earthing set (accessories)",2,2CPX052613R9999,"DIN rail spacing 125 mm/150 mm

Fields for DIN rail devices with DIN rails of 35 x 7,5 mm and N/PE Quick-terminals (1 x ZK224 per field width)

Fields with mounting plates

Fields for terminal blocks with DIN rails of 35 x 7,5 mm insulated mounted (without N/PE Quick-terminals)",715,4,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",36.8,CU24V      Compact Distr.B 2PW 4R IP31,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Cable entry covers

Lock replacement parts

Sheet steel- and transparent doors

Media panels

Distribution panels

CombiLine modules"
CU25V,0,0,1,1,1,615,18,"ComfortLine Compact CU distribution boards for flush and hollow wall mounting*

with distribution panels, frames and sheet steel doors.",120,IK09,"II, insulated

I, grounded in connection with earthing set (accessories)",2,2CPX052614R9999,"DIN rail spacing 125 mm/150 mm

Fields for DIN rail devices with DIN rails of 35 x 7,5 mm and N/PE Quick-terminals (1 x ZK224 per field width)

Fields with mounting plates

Fields for terminal blocks with DIN rails of 35 x 7,5 mm insulated mounted (without N/PE Quick-terminals)",865,5,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",43.5,CU25V      Compact Distr.B 2PW 5R IP31,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Cable entry covers

Lock replacement parts

Sheet steel- and transparent doors

Media panels

Distribution panels

CombiLine modules"
CU26V,0,0,1,1,1,615,20.5,"ComfortLine Compact CU distribution boards for flush and hollow wall mounting*

with distribution panels, frames and sheet steel doors.",144,IK09,"II, insulated

I, grounded in connection with earthing set (accessories)",2,2CPX052615R9999,"DIN rail spacing 125 mm/150 mm

Fields for DIN rail devices with DIN rails of 35 x 7,5 mm and N/PE Quick-terminals (1 x ZK224 per field width)

Fields with mounting plates

Fields for terminal blocks with DIN rails of 35 x 7,5 mm insulated mounted (without N/PE Quick-terminals)",1015,6,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",50.2,CU26V      Compact Distr.B 2PW 6R IP31,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Cable entry covers

Lock replacement parts

Sheet steel- and transparent doors

Media panels

Distribution panels

CombiLine modules"
CU27V,0,0,1,1,1,615,23.5,"ComfortLine Compact CU distribution boards for flush and hollow wall mounting*

with distribution panels, frames and sheet steel doors.",168,IK09,"II, insulated

I, grounded in connection with earthing set (accessories)",2,2CPX052616R9999,"DIN rail spacing 125 mm/150 mm

Fields for DIN rail devices with DIN rails of 35 x 7,5 mm and N/PE Quick-terminals (1 x ZK224 per field width)

Fields with mounting plates

Fields for terminal blocks with DIN rails of 35 x 7,5 mm insulated mounted (without N/PE Quick-terminals)",1165,7,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",56.9,CU27V      Compact Distr.B 2PW 7R IP31,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Cable entry covers

Lock replacement parts

Sheet steel- and transparent doors

Media panels

Distribution panels

CombiLine modules"
CU28V,0,0,1,1,1,615,23.5,"ComfortLine Compact CU distribution boards for flush and hollow wall mounting*

with distribution panels, frames and sheet steel doors.",192,IK09,"II, insulated

I, grounded in connection with earthing set (accessories)",2,2CPX052617R9999,"DIN rail spacing 125 mm/150 mm

Fields for DIN rail devices with DIN rails of 35 x 7,5 mm and N/PE Quick-terminals (1 x ZK224 per field width)

Fields with mounting plates

Fields for terminal blocks with DIN rails of 35 x 7,5 mm insulated mounted (without N/PE Quick-terminals)",1315,8,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",56.9,CU28V      Compact Distr.B 2PW 8R IP31,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Cable entry covers

Lock replacement parts

Sheet steel- and transparent doors

Media panels

Distribution panels

CombiLine modules"
CU34V,0,0,1,1,1,865,21,"ComfortLine Compact CU distribution boards for flush and hollow wall mounting*

with distribution panels, frames and sheet steel doors.",144,IK09,"II, insulated

I, grounded in connection with earthing set (accessories)",3,2CPX052618R9999,"DIN rail spacing 125 mm/150 mm

Fields for DIN rail devices with DIN rails of 35 x 7,5 mm and N/PE Quick-terminals (1 x ZK224 per field width)

Fields with mounting plates

Fields for terminal blocks with DIN rails of 35 x 7,5 mm insulated mounted (without N/PE Quick-terminals)",715,4,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",52.7,CU34V      Compact Distr.B 3PW 4R IP31,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Cable entry covers

Lock replacement parts

Sheet steel- and transparent doors

Media panels

Distribution panels

CombiLine modules"
CU35V,0,0,1,1,1,865,25,"ComfortLine Compact CU distribution boards for flush and hollow wall mounting*

with distribution panels, frames and sheet steel doors.",180,IK09,"II, insulated

I, grounded in connection with earthing set (accessories)",3,2CPX052619R9999,"DIN rail spacing 125 mm/150 mm

Fields for DIN rail devices with DIN rails of 35 x 7,5 mm and N/PE Quick-terminals (1 x ZK224 per field width)

Fields with mounting plates

Fields for terminal blocks with DIN rails of 35 x 7,5 mm insulated mounted (without N/PE Quick-terminals)",865,5,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",61.7,CU35V      Compact Distr.B 3PW 5R IP31,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Cable entry covers

Lock replacement parts

Sheet steel- and transparent doors

Media panels

Distribution panels

CombiLine modules"
CU36V,0,0,1,1,1,865,30,"ComfortLine Compact CU distribution boards for flush and hollow wall mounting*

with distribution panels, frames and sheet steel doors.",216,IK09,"II, insulated

I, grounded in connection with earthing set (accessories)",3,2CPX052620R9999,"DIN rail spacing 125 mm/150 mm

Fields for DIN rail devices with DIN rails of 35 x 7,5 mm and N/PE Quick-terminals (1 x ZK224 per field width)

Fields with mounting plates

Fields for terminal blocks with DIN rails of 35 x 7,5 mm insulated mounted (without N/PE Quick-terminals)",1015,6,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",70.5,CU36V      Compact Distr.B 3PW 6R IP31,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Cable entry covers

Lock replacement parts

Sheet steel- and transparent doors

Media panels

Distribution panels

CombiLine modules"
CU37V,0,0,1,1,1,865,33,"ComfortLine Compact CU distribution boards for flush and hollow wall mounting*

with distribution panels, frames and sheet steel doors.",252,IK09,"II, insulated

I, grounded in connection with earthing set (accessories)",3,2CPX052621R9999,"DIN rail spacing 125 mm/150 mm

Fields for DIN rail devices with DIN rails of 35 x 7,5 mm and N/PE Quick-terminals (1 x ZK224 per field width)

Fields with mounting plates

Fields for terminal blocks with DIN rails of 35 x 7,5 mm insulated mounted (without N/PE Quick-terminals)",1165,7,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",82.1,CU37V      Compact Distr.B 3PW 7R IP31,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Cable entry covers

Lock replacement parts

Sheet steel- and transparent doors

Media panels

Distribution panels

CombiLine modules"
CU45V,0,0,1,1,1,1115,31.5,"ComfortLine Compact CU distribution boards for flush and hollow wall mounting*

with distribution panels, frames and sheet steel doors.",240,IK09,"II, insulated

I, grounded in connection with earthing set (accessories)",4,2CPX052622R9999,"DIN rail spacing 125 mm/150 mm

Fields for DIN rail devices with DIN rails of 35 x 7,5 mm and N/PE Quick-terminals (1 x ZK224 per field width)

Fields with mounting plates

Fields for terminal blocks with DIN rails of 35 x 7,5 mm insulated mounted (without N/PE Quick-terminals)",865,5,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",56.2,CU45V      Compact Distr.B 4PW 5R IP31,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Cable entry covers

Lock replacement parts

Sheet steel- and transparent doors

Media panels

Distribution panels

CombiLine modules"
CU24R,0,0,1,1,1,615,15,"ComfortLine Compact CU distribution boards for flush and hollow wall mounting*

with distribution panels, frames and sheet steel doors.",72,IK09,"II, insulated

I, grounded in connection with earthing set (accessories)",2,2CPX052600R9999,"DIN rail spacing 125 mm/150 mm

Fields for DIN rail devices with DIN rails of 35 x 7,5 mm and N/PE Quick-terminals (1 x ZK224 per field width)

Fields with mounting plates

Fields for terminal blocks with DIN rails of 35 x 7,5 mm insulated mounted (without N/PE Quick-terminals)",715,4,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",36.8,CU24R      Compact DB 2PW 3R IP31 150mm,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Cable entry covers

Lock replacement parts

Sheet steel- and transparent doors

Media panels

Distribution panels

CombiLine modules"
CU25R,0,0,1,1,1,615,18,"ComfortLine Compact CU distribution boards for flush and hollow wall mounting*

with distribution panels, frames and sheet steel doors.",96,IK09,"II, insulated

I, grounded in connection with earthing set (accessories)",2,2CPX052601R9999,"DIN rail spacing 125 mm/150 mm

Fields for DIN rail devices with DIN rails of 35 x 7,5 mm and N/PE Quick-terminals (1 x ZK224 per field width)

Fields with mounting plates

Fields for terminal blocks with DIN rails of 35 x 7,5 mm insulated mounted (without N/PE Quick-terminals)",865,5,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",43.5,CU25R      Compact DB 2PW 4R IP31 150mm,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Cable entry covers

Lock replacement parts

Sheet steel- and transparent doors

Media panels

Distribution panels

CombiLine modules"
CU26R,0,0,1,1,1,615,20.5,"ComfortLine Compact CU distribution boards for flush and hollow wall mounting*

with distribution panels, frames and sheet steel doors.",120,IK09,"II, insulated

I, grounded in connection with earthing set (accessories)",2,2CPX052602R9999,"DIN rail spacing 125 mm/150 mm

Fields for DIN rail devices with DIN rails of 35 x 7,5 mm and N/PE Quick-terminals (1 x ZK224 per field width)

Fields with mounting plates

Fields for terminal blocks with DIN rails of 35 x 7,5 mm insulated mounted (without N/PE Quick-terminals)",1015,6,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",50.2,CU26R      Compact DB 2PW 5R IP31 150mm,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Cable entry covers

Lock replacement parts

Sheet steel- and transparent doors

Media panels

Distribution panels

CombiLine modules"
CU27R,0,0,1,1,1,615,23.5,"ComfortLine Compact CU distribution boards for flush and hollow wall mounting*

with distribution panels, frames and sheet steel doors.",168,IK09,"II, insulated

I, grounded in connection with earthing set (accessories)",2,2CPX052603R9999,"DIN rail spacing 125 mm/150 mm

Fields for DIN rail devices with DIN rails of 35 x 7,5 mm and N/PE Quick-terminals (1 x ZK224 per field width)

Fields with mounting plates

Fields for terminal blocks with DIN rails of 35 x 7,5 mm insulated mounted (without N/PE Quick-terminals)",1165,7,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",56.9,CU27R      Compact DB 2PW 6R IP31 150mm,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Cable entry covers

Lock replacement parts

Sheet steel- and transparent doors

Media panels

Distribution panels

CombiLine modules"
CU28R,0,0,1,1,1,615,26,"ComfortLine Compact CU distribution boards for flush and hollow wall mounting*

with distribution panels, frames and sheet steel doors.",192,IK09,"II, insulated

I, grounded in connection with earthing set (accessories)",2,2CPX052604R9999,"DIN rail spacing 125 mm/150 mm

Fields for DIN rail devices with DIN rails of 35 x 7,5 mm and N/PE Quick-terminals (1 x ZK224 per field width)

Fields with mounting plates

Fields for terminal blocks with DIN rails of 35 x 7,5 mm insulated mounted (without N/PE Quick-terminals)",1315,8,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",63.6,CU28R      Compact DB 2PW 7R IP31 150mm,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Cable entry covers

Lock replacement parts

Sheet steel- and transparent doors

Media panels

Distribution panels

CombiLine modules"
CU36R,0,0,1,1,1,865,30,"ComfortLine Compact CU distribution boards for flush and hollow wall mounting*

with distribution panels, frames and sheet steel doors.",216,IK09,"II, insulated

I, grounded in connection with earthing set (accessories)",3,2CPX052605R9999,"DIN rail spacing 125 mm/150 mm

Fields for DIN rail devices with DIN rails of 35 x 7,5 mm and N/PE Quick-terminals (1 x ZK224 per field width)

Fields with mounting plates

Fields for terminal blocks with DIN rails of 35 x 7,5 mm insulated mounted (without N/PE Quick-terminals)",1015,6,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",70.5,CU36R      Compact DB 3PW 5R IP31 150mm,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Cable entry covers

Lock replacement parts

Sheet steel- and transparent doors

Media panels

Distribution panels

CombiLine modules"
CU37R,0,0,1,1,1,865,33,"ComfortLine Compact CU distribution boards for flush and hollow wall mounting*

with distribution panels, frames and sheet steel doors.",288,IK09,"II, insulated

I, grounded in connection with earthing set (accessories)",3,2CPX052606R9999,"DIN rail spacing 125 mm/150 mm

Fields for DIN rail devices with DIN rails of 35 x 7,5 mm and N/PE Quick-terminals (1 x ZK224 per field width)

Fields with mounting plates

Fields for terminal blocks with DIN rails of 35 x 7,5 mm insulated mounted (without N/PE Quick-terminals)",1165,7,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",82.1,CU37R      Compact DB 3PW 6R IP31 150mm,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Cable entry covers

Lock replacement parts

Sheet steel- and transparent doors

Media panels

Distribution panels

CombiLine modules"
CU25K,0,0,1,1,1,615,18,"ComfortLine Compact CU distribution boards for flush and hollow wall mounting*

with distribution panels, frames and sheet steel doors.",72,IK09,"II, insulated

I, grounded in connection with earthing set (accessories)",2,2CPX052623R9999,"DIN rail spacing 125 mm/150 mm

Fields for DIN rail devices with DIN rails of 35 x 7,5 mm and N/PE Quick-terminals (1 x ZK224 per field width)

Fields with mounting plates

Fields for terminal blocks with DIN rails of 35 x 7,5 mm insulated mounted (without N/PE Quick-terminals)",865,5,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",43.5,CU25K      Compact DB 2PW 3R term.space,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Cable entry covers

Lock replacement parts

Sheet steel- and transparent doors

Media panels

Distribution panels

CombiLine modules"
CU26K,0,0,1,1,1,615,21.5,"ComfortLine Compact CU distribution boards for flush and hollow wall mounting*

with distribution panels, frames and sheet steel doors.",96,IK09,"II, insulated

I, grounded in connection with earthing set (accessories)",2,2CPX052624R9999,"DIN rail spacing 125 mm/150 mm

Fields for DIN rail devices with DIN rails of 35 x 7,5 mm and N/PE Quick-terminals (1 x ZK224 per field width)

Fields with mounting plates

Fields for terminal blocks with DIN rails of 35 x 7,5 mm insulated mounted (without N/PE Quick-terminals)",1015,6,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",50.2,CU26K      Compact DB 2PW 4R term.space,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Cable entry covers

Lock replacement parts

Sheet steel- and transparent doors

Media panels

Distribution panels

CombiLine modules"
CU27K,0,0,1,1,1,615,23.5,"ComfortLine Compact CU distribution boards for flush and hollow wall mounting*

with distribution panels, frames and sheet steel doors.",96,IK09,"II, insulated

I, grounded in connection with earthing set (accessories)",2,2CPX052625R9999,"DIN rail spacing 125 mm/150 mm

Fields for DIN rail devices with DIN rails of 35 x 7,5 mm and N/PE Quick-terminals (1 x ZK224 per field width)

Fields with mounting plates

Fields for terminal blocks with DIN rails of 35 x 7,5 mm insulated mounted (without N/PE Quick-terminals)",1165,7,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",56.9,CU27K      Compact DB 2PW 5R term.space,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Cable entry covers

Lock replacement parts

Sheet steel- and transparent doors

Media panels

Distribution panels

CombiLine modules"
CU35K,0,0,1,1,1,865,25.5,"ComfortLine Compact CU distribution boards for flush and hollow wall mounting*

with distribution panels, frames and sheet steel doors.",108,IK09,"II, insulated

I, grounded in connection with earthing set (accessories)",3,2CPX052626R9999,"DIN rail spacing 125 mm/150 mm

Fields for DIN rail devices with DIN rails of 35 x 7,5 mm and N/PE Quick-terminals (1 x ZK224 per field width)

Fields with mounting plates

Fields for terminal blocks with DIN rails of 35 x 7,5 mm insulated mounted (without N/PE Quick-terminals)",865,5,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",61.7,CU35K      Compact DB 3PW 3R term.space,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Cable entry covers

Lock replacement parts

Sheet steel- and transparent doors

Media panels

Distribution panels

CombiLine modules"
CU36K,0,0,1,1,1,865,30.5,"ComfortLine Compact CU distribution boards for flush and hollow wall mounting*

with distribution panels, frames and sheet steel doors.",144,IK09,"II, insulated

I, grounded in connection with earthing set (accessories)",3,2CPX052627R9999,"DIN rail spacing 125 mm/150 mm

Fields for DIN rail devices with DIN rails of 35 x 7,5 mm and N/PE Quick-terminals (1 x ZK224 per field width)

Fields with mounting plates

Fields for terminal blocks with DIN rails of 35 x 7,5 mm insulated mounted (without N/PE Quick-terminals)",1015,6,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",70.5,CU36K      Compact DB 3PW 4R term.space,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Cable entry covers

Lock replacement parts

Sheet steel- and transparent doors

Media panels

Distribution panels

CombiLine modules"
CU37K,0,0,1,1,1,865,33,"ComfortLine Compact CU distribution boards for flush and hollow wall mounting*

with distribution panels, frames and sheet steel doors.",144,IK09,"II, insulated

I, grounded in connection with earthing set (accessories)",3,2CPX052628R9999,"DIN rail spacing 125 mm/150 mm

Fields for DIN rail devices with DIN rails of 35 x 7,5 mm and N/PE Quick-terminals (1 x ZK224 per field width)

Fields with mounting plates

Fields for terminal blocks with DIN rails of 35 x 7,5 mm insulated mounted (without N/PE Quick-terminals)",1165,57,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",82.1,CU37K      Compact DB 3PW 5R term.space,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Cable entry covers

Lock replacement parts

Sheet steel- and transparent doors

Media panels

Distribution panels

CombiLine modules"
CU46K,0,0,1,1,1,1115,37.5,"ComfortLine Compact CU distribution boards for flush and hollow wall mounting*

with distribution panels, frames and sheet steel doors.",144,IK09,"II, insulated

I, grounded in connection with earthing set (accessories)",4,2CPX052629R9999,"DIN rail spacing 125 mm/150 mm

Fields for DIN rail devices with DIN rails of 35 x 7,5 mm and N/PE Quick-terminals (1 x ZK224 per field width)

Fields with mounting plates

Fields for terminal blocks with DIN rails of 35 x 7,5 mm insulated mounted (without N/PE Quick-terminals)",1015,6,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",63.9,CU46K      Compact DB 4PW 4R term.space,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Cable entry covers

Lock replacement parts

Sheet steel- and transparent doors

Media panels

Distribution panels

CombiLine modules"
CU24VP,0,0,1,1,1,615,19,"ComfortLine Compact CU distribution boards for flush and hollow wall mounting*

with distribution panels, frames and sheet steel doors.",48,IK09,"II, insulated

I, grounded in connection with earthing set (accessories)",2,2CPX052685R9999,"DIN rail spacing 125 mm/150 mm

Fields for DIN rail devices with DIN rails of 35 x 7,5 mm and N/PE Quick-terminals (1 x ZK224 per field width)

Fields with mounting plates

Fields for terminal blocks with DIN rails of 35 x 7,5 mm insulated mounted (without N/PE Quick-terminals)",715,4,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",36.8,CU24VP     Comp.DB 2PW 4R mounting plate,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Cable entry covers

Lock replacement parts

Sheet steel- and transparent doors

Media panels

Distribution panels

CombiLine modules"
CU35VP,0,0,1,1,1,865,29.5,"ComfortLine Compact CU distribution boards for flush and hollow wall mounting*

with distribution panels, frames and sheet steel doors.",120,IK09,"II, insulated

I, grounded in connection with earthing set (accessories)",3,2CPX052686R9999,"DIN rail spacing 125 mm/150 mm

Fields for DIN rail devices with DIN rails of 35 x 7,5 mm and N/PE Quick-terminals (1 x ZK224 per field width)

Fields with mounting plates

Fields for terminal blocks with DIN rails of 35 x 7,5 mm insulated mounted (without N/PE Quick-terminals)",865,5,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount","61,7",CU35VP     Comp.DB 3PW 5R mounting plate,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Cable entry covers

Lock replacement parts

Sheet steel- and transparent doors

Media panels

Distribution panels

CombiLine modules"
CU14B,0,0,0,1,0,365,6.5,"ComfortLine Compact CU distribution boards. For flush and hollow wall mounting*,

empty cabinets with blend frame, without doors.",48,IK09 With sheet steel door; IK07 semi-transparent/transparent doors,"II, insulated

I, grounded in connection with earthing set (accessories)",1,2CPX052647R9999,"Prepared for expansion with CombiLine modules, distribution panels, and media panels

Without N/PE Quick-Terminal",715,4,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

With cable pull/tension mount",22.1,CU14B      Comp.DB 1PW 4R empty wo.door,"Cabinet with frame, without door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Hollow wall mounting kit for flush-mounted cabinets

Sheet steel and transparent doors

Lock replacement parts

Media fields

Distribution panels

CombiLine modules"
CU15B,0,0,0,1,0,365,7.5,"ComfortLine Compact CU distribution boards. For flush and hollow wall mounting*,

empty cabinets with blend frame, without doors.",60,IK09 With sheet steel door; IK07 semi-transparent/transparent doors,"II, insulated

I, grounded in connection with earthing set (accessories)",1,2CPX052648R9999,"Prepared for expansion with CombiLine modules, distribution panels, and media panels

Without N/PE Quick-Terminal",865,5,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

With cable pull/tension mount",26.5,CU15B      Comp.DB 1PW 5R empty wo.door,"Cabinet with frame, without door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Hollow wall mounting kit for flush-mounted cabinets

Sheet steel and transparent doors

Lock replacement parts

Media fields

Distribution panels

CombiLine modules"
CU16B,0,0,0,1,0,365,8.5,"ComfortLine Compact CU distribution boards. For flush and hollow wall mounting*,

empty cabinets with blend frame, without doors.",72,IK09 With sheet steel door; IK07 semi-transparent/transparent doors,"II, insulated

I, grounded in connection with earthing set (accessories)",1,2CPX052649R9999,"Prepared for expansion with CombiLine modules, distribution panels, and media panels

Without N/PE Quick-Terminal",1015,6,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

With cable pull/tension mount",30.9,CU16B      Comp.DB 1PW 6R empty wo.door,"Cabinet with frame, without door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Hollow wall mounting kit for flush-mounted cabinets

Sheet steel and transparent doors

Lock replacement parts

Media fields

Distribution panels

CombiLine modules"
CU17B,0,0,0,1,0,365,10,"ComfortLine Compact CU distribution boards. For flush and hollow wall mounting*,

empty cabinets with blend frame, without doors.",84,IK09 With sheet steel door; IK07 semi-transparent/transparent doors,"II, insulated

I, grounded in connection with earthing set (accessories)",1,2CPX052650R9999,"Prepared for expansion with CombiLine modules, distribution panels, and media panels

Without N/PE Quick-Terminal",1165,7,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

With cable pull/tension mount",35.5,CU17B      Comp.DB 1PW 7R empty wo.door,"Cabinet with frame, without door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Hollow wall mounting kit for flush-mounted cabinets

Sheet steel and transparent doors

Lock replacement parts

Media fields

Distribution panels

CombiLine modules"
CU18B,0,0,0,1,0,365,10.5,"ComfortLine Compact CU distribution boards. For flush and hollow wall mounting*,

empty cabinets with blend frame, without doors.",86,IK09 With sheet steel door; IK07 semi-transparent/transparent doors,"II, insulated

I, grounded in connection with earthing set (accessories)",1,2CPX052651R9999,"Prepared for expansion with CombiLine modules, distribution panels, and media panels

Without N/PE Quick-Terminal",1315,8,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

With cable pull/tension mount",39.9,CU18B      Comp.DB 1PW 8R empty wo.door,"Cabinet with frame, without door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Hollow wall mounting kit for flush-mounted cabinets

Sheet steel and transparent doors

Lock replacement parts

Media fields

Distribution panels

CombiLine modules"
CU23B,0,0,0,1,0,615,7.5,"ComfortLine Compact CU distribution boards. For flush and hollow wall mounting*,

empty cabinets with blend frame, without doors.",72,IK09 With sheet steel door; IK07 semi-transparent/transparent doors,"II, insulated

I, grounded in connection with earthing set (accessories)",2,2CPX052652R9999,"Prepared for expansion with CombiLine modules, distribution panels, and media panels

Without N/PE Quick-Terminal",565,3,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

With cable pull/tension mount",35.1,CU23B      Comp.DB 2PW 3R empty wo.door,"Cabinet with frame, without door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Hollow wall mounting kit for flush-mounted cabinets

Sheet steel and transparent doors

Lock replacement parts

Media fields

Distribution panels

CombiLine modules"
CU24B,0,0,0,1,0,615,9,"ComfortLine Compact CU distribution boards. For flush and hollow wall mounting*,

empty cabinets with blend frame, without doors.",96,IK09 With sheet steel door; IK07 semi-transparent/transparent doors,"II, insulated

I, grounded in connection with earthing set (accessories)",2,2CPX052653R9999,"Prepared for expansion with CombiLine modules, distribution panels, and media panels

Without N/PE Quick-Terminal",715,4,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

With cable pull/tension mount",36.8,CU24B      Comp.DB 2PW 4R empty wo.door,"Cabinet with frame, without door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Hollow wall mounting kit for flush-mounted cabinets

Sheet steel and transparent doors

Lock replacement parts

Media fields

Distribution panels

CombiLine modules"
CU25B,0,0,0,1,0,615,10.5,"ComfortLine Compact CU distribution boards. For flush and hollow wall mounting*,

empty cabinets with blend frame, without doors.",120,IK09 With sheet steel door; IK07 semi-transparent/transparent doors,"II, insulated

I, grounded in connection with earthing set (accessories)",2,2CPX052654R9999,"Prepared for expansion with CombiLine modules, distribution panels, and media panels

Without N/PE Quick-Terminal",865,5,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

With cable pull/tension mount",43.5,CU25B      Comp.DB 2PW 5R empty wo.door,"Cabinet with frame, without door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Hollow wall mounting kit for flush-mounted cabinets

Sheet steel and transparent doors

Lock replacement parts

Media fields

Distribution panels

CombiLine modules"
CU26B,0,0,0,1,0,615,12,"ComfortLine Compact CU distribution boards. For flush and hollow wall mounting*,

empty cabinets with blend frame, without doors.",144,IK09 With sheet steel door; IK07 semi-transparent/transparent doors,"II, insulated

I, grounded in connection with earthing set (accessories)",2,2CPX052655R9999,"Prepared for expansion with CombiLine modules, distribution panels, and media panels

Without N/PE Quick-Terminal",1015,6,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

With cable pull/tension mount",50.2,CU26B      Comp.DB 2PW 6R empty wo.door,"Cabinet with frame, without door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Hollow wall mounting kit for flush-mounted cabinets

Sheet steel and transparent doors

Lock replacement parts

Media fields

Distribution panels

CombiLine modules"
CU27B,0,0,0,1,0,615,13.5,"ComfortLine Compact CU distribution boards. For flush and hollow wall mounting*,

empty cabinets with blend frame, without doors.",168,IK09 With sheet steel door; IK07 semi-transparent/transparent doors,"II, insulated

I, grounded in connection with earthing set (accessories)",2,2CPX052656R9999,"Prepared for expansion with CombiLine modules, distribution panels, and media panels

Without N/PE Quick-Terminal",1165,7,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

With cable pull/tension mount",56.9,CU27B      Comp.DB 2PW 7R empty wo.door,"Cabinet with frame, without door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Hollow wall mounting kit for flush-mounted cabinets

Sheet steel and transparent doors

Lock replacement parts

Media fields

Distribution panels

CombiLine modules"
CU28B,0,0,0,1,0,615,14,"ComfortLine Compact CU distribution boards. For flush and hollow wall mounting*,

empty cabinets with blend frame, without doors.",192,IK09 With sheet steel door; IK07 semi-transparent/transparent doors,"II, insulated

I, grounded in connection with earthing set (accessories)",2,2CPX052657R9999,"Prepared for expansion with CombiLine modules, distribution panels, and media panels

Without N/PE Quick-Terminal",1315,8,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

With cable pull/tension mount",63.6,CU28B      Comp.DB 2PW 8R empty wo.door,"Cabinet with frame, without door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Hollow wall mounting kit for flush-mounted cabinets

Sheet steel and transparent doors

Lock replacement parts

Media fields

Distribution panels

CombiLine modules"
CU34B,0,0,0,1,0,865,11.5,"ComfortLine Compact CU distribution boards. For flush and hollow wall mounting*,

empty cabinets with blend frame, without doors.",144,IK09 With sheet steel door; IK07 semi-transparent/transparent doors,"II, insulated

I, grounded in connection with earthing set (accessories)",3,2CPX052658R9999,"Prepared for expansion with CombiLine modules, distribution panels, and media panels

Without N/PE Quick-Terminal",715,4,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

With cable pull/tension mount",52.7,CU34B      Comp.DB 3PW 4R empty wo.door,"Cabinet with frame, without door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Hollow wall mounting kit for flush-mounted cabinets

Sheet steel and transparent doors

Lock replacement parts

Media fields

Distribution panels

CombiLine modules"
CU35B,0,0,0,1,0,865,13.5,"ComfortLine Compact CU distribution boards. For flush and hollow wall mounting*,

empty cabinets with blend frame, without doors.",180,IK09 With sheet steel door; IK07 semi-transparent/transparent doors,"II, insulated

I, grounded in connection with earthing set (accessories)",3,2CPX052659R9999,"Prepared for expansion with CombiLine modules, distribution panels, and media panels

Without N/PE Quick-Terminal",865,5,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

With cable pull/tension mount",61.7,CU35B      Comp.DB 3PW 5R empty wo.door,"Cabinet with frame, without door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Hollow wall mounting kit for flush-mounted cabinets

Sheet steel and transparent doors

Lock replacement parts

Media fields

Distribution panels

CombiLine modules"
CU36B,0,0,0,1,0,865,16,"ComfortLine Compact CU distribution boards. For flush and hollow wall mounting*,

empty cabinets with blend frame, without doors.",216,IK09 With sheet steel door; IK07 semi-transparent/transparent doors,"II, insulated

I, grounded in connection with earthing set (accessories)",3,2CPX052660R9999,"Prepared for expansion with CombiLine modules, distribution panels, and media panels

Without N/PE Quick-Terminal",1015,6,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

With cable pull/tension mount",70.5,CU36B      Comp.DB 3PW 6R empty wo.door,"Cabinet with frame, without door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Hollow wall mounting kit for flush-mounted cabinets

Sheet steel and transparent doors

Lock replacement parts

Media fields

Distribution panels

CombiLine modules"
CU37B,0,0,0,1,0,865,17,"ComfortLine Compact CU distribution boards. For flush and hollow wall mounting*,

empty cabinets with blend frame, without doors.",252,IK09 With sheet steel door; IK07 semi-transparent/transparent doors,"II, insulated

I, grounded in connection with earthing set (accessories)",3,2CPX052661R9999,"Prepared for expansion with CombiLine modules, distribution panels, and media panels

Without N/PE Quick-Terminal",1165,7,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

With cable pull/tension mount",82.1,CU37B      Comp.DB 3PW 7R empty wo.door,"Cabinet with frame, without door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Hollow wall mounting kit for flush-mounted cabinets

Sheet steel and transparent doors

Lock replacement parts

Media fields

Distribution panels

CombiLine modules"
CU45B,0,0,0,1,0,1115,16.5,"ComfortLine Compact CU distribution boards. For flush and hollow wall mounting*,

empty cabinets with blend frame, without doors.",240,IK09 With sheet steel door; IK07 semi-transparent/transparent doors,"II, insulated

I, grounded in connection with earthing set (accessories)",4,2CPX052662R9999,"Prepared for expansion with CombiLine modules, distribution panels, and media panels

Without N/PE Quick-Terminal",865,5,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

With cable pull/tension mount",56.2,CU45B      Comp.DB 4PW 5R empty wo.door,"Cabinet with frame, without door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Hollow wall mounting kit for flush-mounted cabinets

Sheet steel and transparent doors

Lock replacement parts

Media fields

Distribution panels

CombiLine modules"
CU46B,0,0,0,1,0,1115,18.5,"ComfortLine Compact CU distribution boards. For flush and hollow wall mounting*,

empty cabinets with blend frame, without doors.",288,IK09 With sheet steel door; IK07 semi-transparent/transparent doors,"II, insulated

I, grounded in connection with earthing set (accessories)",4,2CPX052663R9999,"Prepared for expansion with CombiLine modules, distribution panels, and media panels

Without N/PE Quick-Terminal",1015,6,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

With cable pull/tension mount",63.9,CU46B      Comp.DB 4PW 6R empty wo.door,"Cabinet with frame, without door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Hollow wall mounting kit for flush-mounted cabinets

Sheet steel and transparent doors

Lock replacement parts

Media fields

Distribution panels

CombiLine modules"
CU24VM,0,0,1,1,1,615,15.5,"ComfortLine Compact CU distribution boards For flush and hollow wall mounting*

with media unit with blend frame and multiple door options.",48,IK09 with sheet steel door; IK07 semi-transparent/transparent doors,"II, insulated

I, grounded in connection with earthing set (accessories)",2,2CPX052664R9999,"DIN rail spacing 125 mm

Fields for DIN rail devices with DIN rails of 35 x 7,5 mm and N/PE Quick-terminals (1 x ZK224 per field width)

Pre-assembled perforated sheet mounting plate",715,4,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",41.7,CU24VM     Compact DB 2PW 4R media,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Hollow wall set for flush-mounted cabinets

Lock replacement parts

Sockets

Patch panel"
CU25VM,0,0,1,1,1,615,18.5,"ComfortLine Compact CU distribution boards For flush and hollow wall mounting*

with media unit with blend frame and multiple door options.",60,IK09 with sheet steel door; IK07 semi-transparent/transparent doors,"II, insulated

I, grounded in connection with earthing set (accessories)",2,2CPX052665R9999,"DIN rail spacing 125 mm

Fields for DIN rail devices with DIN rails of 35 x 7,5 mm and N/PE Quick-terminals (1 x ZK224 per field width)

Pre-assembled perforated sheet mounting plate",865,5,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",50,CU25VM     Compact DB 2PW 5R media,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Hollow wall set for flush-mounted cabinets

Lock replacement parts

Sockets

Patch panel"
CU26VM,0,0,1,1,1,615,21.5,"ComfortLine Compact CU distribution boards For flush and hollow wall mounting*

with media unit with blend frame and multiple door options.",72,IK09 with sheet steel door; IK07 semi-transparent/transparent doors,"II, insulated

I, grounded in connection with earthing set (accessories)",2,2CPX052666R9999,"DIN rail spacing 125 mm

Fields for DIN rail devices with DIN rails of 35 x 7,5 mm and N/PE Quick-terminals (1 x ZK224 per field width)

Pre-assembled perforated sheet mounting plate",1015,6,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",58.6,CU26VM     Compact DB 2PW 6R media,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Hollow wall set for flush-mounted cabinets

Lock replacement parts

Sockets

Patch panel"
CU27VM,0,0,1,1,1,615,24.5,"ComfortLine Compact CU distribution boards For flush and hollow wall mounting*

with media unit with blend frame and multiple door options.",84,IK09 with sheet steel door; IK07 semi-transparent/transparent doors,"II, insulated

I, grounded in connection with earthing set (accessories)",2,2CPX052667R9999,"DIN rail spacing 125 mm

Fields for DIN rail devices with DIN rails of 35 x 7,5 mm and N/PE Quick-terminals (1 x ZK224 per field width)

Pre-assembled perforated sheet mounting plate",1165,7,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",67,CU27VM     Compact DB 2PW 7R media,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Hollow wall set for flush-mounted cabinets

Lock replacement parts

Sockets

Patch panel"
CU34VM,0,0,1,1,1,865,21,"ComfortLine Compact CU distribution boards For flush and hollow wall mounting*

with media unit with blend frame and multiple door options.",96,IK09 with sheet steel door; IK07 semi-transparent/transparent doors,"II, insulated

I, grounded in connection with earthing set (accessories)",3,2CPX052668R9999,"DIN rail spacing 125 mm

Fields for DIN rail devices with DIN rails of 35 x 7,5 mm and N/PE Quick-terminals (1 x ZK224 per field width)

Pre-assembled perforated sheet mounting plate",715,4,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",56.2,CU34VM     Compact DB 3PW 4R media,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Hollow wall set for flush-mounted cabinets

Lock replacement parts

Sockets

Patch panel"
CU35VM,0,0,1,1,1,865,25,"ComfortLine Compact CU distribution boards For flush and hollow wall mounting*

with media unit with blend frame and multiple door options.",120,IK09 with sheet steel door; IK07 semi-transparent/transparent doors,"II, insulated

I, grounded in connection with earthing set (accessories)",3,2CPX052669R9999,"DIN rail spacing 125 mm

Fields for DIN rail devices with DIN rails of 35 x 7,5 mm and N/PE Quick-terminals (1 x ZK224 per field width)

Pre-assembled perforated sheet mounting plate",865,5,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",66.8,CU35VM     Compact DB 3PW 5R media,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Hollow wall set for flush-mounted cabinets

Lock replacement parts

Sockets

Patch panel"
CU36VM,0,0,1,1,1,865,30,"ComfortLine Compact CU distribution boards For flush and hollow wall mounting*

with media unit with blend frame and multiple door options.",144,IK09 with sheet steel door; IK07 semi-transparent/transparent doors,"II, insulated

I, grounded in connection with earthing set (accessories)",3,2CPX052670R9999,"DIN rail spacing 125 mm

Fields for DIN rail devices with DIN rails of 35 x 7,5 mm and N/PE Quick-terminals (1 x ZK224 per field width)

Pre-assembled perforated sheet mounting plate",1015,6,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",77.7,CU36VM     Compact DB 3PW 6R media,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Hollow wall set for flush-mounted cabinets

Lock replacement parts

Sockets

Patch panel"
CU24VML,0,1,0,1,1,615,15.5,"ComfortLine Compact CU distribution boards for flush and hollow wall mounting*

with distribution panels, frames and sheet steel doors.",48,IK09,"II, insulated

I, grounded in connection with earthing set (accessories)",2,2CPX052671R9999,"DIN rail spacing 125 mm/150 mm

Fields for DIN rail devices with DIN rails of 35 x 7,5 mm and N/PE Quick-terminals (1 x ZK224 per field width)

Fields with mounting plates

Fields for terminal blocks with DIN rails of 35 x 7,5 mm insulated mounted (without N/PE Quick-terminals)",715,4,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",41.7,CU24VML    Compact DB 2PW 4R media vent.,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Cable entry covers

Lock replacement parts

Sheet steel- and transparent doors

Media panels

Distribution panels

CombiLine modules"
CU25VML,0,1,0,1,1,615,18.5,"ComfortLine Compact CU distribution boards for flush and hollow wall mounting*

with distribution panels, frames and sheet steel doors.",60,IK09,"II, insulated

I, grounded in connection with earthing set (accessories)",2,2CPX052672R9999,"DIN rail spacing 125 mm/150 mm

Fields for DIN rail devices with DIN rails of 35 x 7,5 mm and N/PE Quick-terminals (1 x ZK224 per field width)

Fields with mounting plates

Fields for terminal blocks with DIN rails of 35 x 7,5 mm insulated mounted (without N/PE Quick-terminals)",865,5,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",50,CU25VML    Compact DB 2PW 5R media vent.,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Cable entry covers

Lock replacement parts

Sheet steel- and transparent doors

Media panels

Distribution panels

CombiLine modules"
CU26VML,0,1,0,1,1,615,21.5,"ComfortLine Compact CU distribution boards for flush and hollow wall mounting*

with distribution panels, frames and sheet steel doors.",72,IK09,"II, insulated

I, grounded in connection with earthing set (accessories)",2,2CPX052673R9999,"DIN rail spacing 125 mm/150 mm

Fields for DIN rail devices with DIN rails of 35 x 7,5 mm and N/PE Quick-terminals (1 x ZK224 per field width)

Fields with mounting plates

Fields for terminal blocks with DIN rails of 35 x 7,5 mm insulated mounted (without N/PE Quick-terminals)",1015,6,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",58.6,CU26VML    Compact DB 2PW 6R media vent.,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Cable entry covers

Lock replacement parts

Sheet steel- and transparent doors

Media panels

Distribution panels

CombiLine modules"
CU27VML,0,1,0,1,1,615,24.5,"ComfortLine Compact CU distribution boards for flush and hollow wall mounting*

with distribution panels, frames and sheet steel doors.",84,IK09,"II, insulated

I, grounded in connection with earthing set (accessories)",2,2CPX052674R9999,"DIN rail spacing 125 mm/150 mm

Fields for DIN rail devices with DIN rails of 35 x 7,5 mm and N/PE Quick-terminals (1 x ZK224 per field width)

Fields with mounting plates

Fields for terminal blocks with DIN rails of 35 x 7,5 mm insulated mounted (without N/PE Quick-terminals)",1165,7,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",67,CU27VML    Compact DB 2PW 7R media vent.,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Cable entry covers

Lock replacement parts

Sheet steel- and transparent doors

Media panels

Distribution panels

CombiLine modules"
CU34VML,0,1,0,1,1,865,21,"ComfortLine Compact CU distribution boards for flush and hollow wall mounting*

with distribution panels, frames and sheet steel doors.",96,IK09,"II, insulated

I, grounded in connection with earthing set (accessories)",3,2CPX052675R9999,"DIN rail spacing 125 mm/150 mm

Fields for DIN rail devices with DIN rails of 35 x 7,5 mm and N/PE Quick-terminals (1 x ZK224 per field width)

Fields with mounting plates

Fields for terminal blocks with DIN rails of 35 x 7,5 mm insulated mounted (without N/PE Quick-terminals)",715,4,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",56.2,CU34VML    Compact DB 3PW 4R media vent.,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Cable entry covers

Lock replacement parts

Sheet steel- and transparent doors

Media panels

Distribution panels

CombiLine modules"
CU35VML,0,1,0,1,1,865,25,"ComfortLine Compact CU distribution boards for flush and hollow wall mounting*

with distribution panels, frames and sheet steel doors.",120,IK09,"II, insulated

I, grounded in connection with earthing set (accessories)",3,2CPX052676R9999,"DIN rail spacing 125 mm/150 mm

Fields for DIN rail devices with DIN rails of 35 x 7,5 mm and N/PE Quick-terminals (1 x ZK224 per field width)

Fields with mounting plates

Fields for terminal blocks with DIN rails of 35 x 7,5 mm insulated mounted (without N/PE Quick-terminals)",865,5,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",66.8,CU35VML    Compact DB 3PW 5R media vent.,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Cable entry covers

Lock replacement parts

Sheet steel- and transparent doors

Media panels

Distribution panels

CombiLine modules"
CU36VML,0,1,0,1,1,865,29.5,"ComfortLine Compact CU distribution boards for flush and hollow wall mounting*

with distribution panels, frames and sheet steel doors.",144,IK09,"II, insulated

I, grounded in connection with earthing set (accessories)",3,2CPX052677R9999,"DIN rail spacing 125 mm/150 mm

Fields for DIN rail devices with DIN rails of 35 x 7,5 mm and N/PE Quick-terminals (1 x ZK224 per field width)

Fields with mounting plates

Fields for terminal blocks with DIN rails of 35 x 7,5 mm insulated mounted (without N/PE Quick-terminals)",1015,6,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",77.7,CU36VML    Compact DB 3PW 6R media vent.,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Cable entry covers

Lock replacement parts

Sheet steel- and transparent doors

Media panels

Distribution panels

CombiLine modules"
CU24VMW,1,0,0,1,1,615,24.5,"ComfortLine Compact CU distribution boards for flush and hollow wall mounting*

with distribution panels, frames and sheet steel doors.",48,IK09,"II, insulated

I, grounded in connection with earthing set (accessories)",2,2CPX052678R9999,"DIN rail spacing 125 mm/150 mm

Fields for DIN rail devices with DIN rails of 35 x 7,5 mm and N/PE Quick-terminals (1 x ZK224 per field width)

Fields with mounting plates

Fields for terminal blocks with DIN rails of 35 x 7,5 mm insulated mounted (without N/PE Quick-terminals)",715,4,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",41.7,CU24VMW    Compact DB 2PW 4R media WiFi,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Cable entry covers

Lock replacement parts

Sheet steel- and transparent doors

Media panels

Distribution panels

CombiLine modules"
CU25VMW,0,0,1,0,0,615,15,"ComfortLine Compact CU distribution boards.

For flush and hollow wall mounting*, with distribution panels and design frames.",96,IK09,"II, insulated",2,2CPX052687R9999,"DIN rail spacing 125 mm

Fields for DIN rail devices with DIN rails of 35 x 7,5 mm and N/PE Quick-terminals (1 x ZK224 per field width)",715,4,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

Interchangeable design frames, brushed aluminium with glass insert

120° door opening angle

Interchangeable design frame with magnetic closure

With cable pull/tension mount",36.8,CU25VMW    Compact DB 2PW 5R media WiFi,"Cabinet with blend frame and interchangeable design frame

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,Hollow wall set for flush-mounted cabinets
CU26VMW,1,0,0,1,1,615,20,"ComfortLine Compact CU distribution boards for flush and hollow wall mounting*

with distribution panels, frames and sheet steel doors.",72,IK09,"II, insulated

I, grounded in connection with earthing set (accessories)",2,2CPX052680R9999,"DIN rail spacing 125 mm/150 mm

Fields for DIN rail devices with DIN rails of 35 x 7,5 mm and N/PE Quick-terminals (1 x ZK224 per field width)

Fields with mounting plates

Fields for terminal blocks with DIN rails of 35 x 7,5 mm insulated mounted (without N/PE Quick-terminals)",1015,6,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",58.6,CU26VMW    Compact DB 2PW 6R media WiFi,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Cable entry covers

Lock replacement parts

Sheet steel- and transparent doors

Media panels

Distribution panels

CombiLine modules"
CU27VMW,1,0,0,1,1,615,23,"ComfortLine Compact CU distribution boards for flush and hollow wall mounting*

with distribution panels, frames and sheet steel doors.",84,IK09,"II, insulated

I, grounded in connection with earthing set (accessories)",2,2CPX052681R9999,"DIN rail spacing 125 mm/150 mm

Fields for DIN rail devices with DIN rails of 35 x 7,5 mm and N/PE Quick-terminals (1 x ZK224 per field width)

Fields with mounting plates

Fields for terminal blocks with DIN rails of 35 x 7,5 mm insulated mounted (without N/PE Quick-terminals)",1165,7,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",67,CU27VMW    Compact DB 2PW 7R media WiFi,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Cable entry covers

Lock replacement parts

Sheet steel- and transparent doors

Media panels

Distribution panels

CombiLine modules"
CU34VMW,1,0,0,1,1,865,20,"ComfortLine Compact CU distribution boards for flush and hollow wall mounting*

with distribution panels, frames and sheet steel doors.",96,IK09,"II, insulated

I, grounded in connection with earthing set (accessories)",3,2CPX052682R9999,"DIN rail spacing 125 mm/150 mm

Fields for DIN rail devices with DIN rails of 35 x 7,5 mm and N/PE Quick-terminals (1 x ZK224 per field width)

Fields with mounting plates

Fields for terminal blocks with DIN rails of 35 x 7,5 mm insulated mounted (without N/PE Quick-terminals)",715,4,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",56.2,CU34VMW    Compact DB 3PW 4R media WiFi,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Cable entry covers

Lock replacement parts

Sheet steel- and transparent doors

Media panels

Distribution panels

CombiLine modules"
CU35VMW,1,0,0,1,1,865,24,"ComfortLine Compact CU distribution boards for flush and hollow wall mounting*

with distribution panels, frames and sheet steel doors.",120,IK09,"II, insulated

I, grounded in connection with earthing set (accessories)",3,2CPX052683R9999,"DIN rail spacing 125 mm/150 mm

Fields for DIN rail devices with DIN rails of 35 x 7,5 mm and N/PE Quick-terminals (1 x ZK224 per field width)

Fields with mounting plates

Fields for terminal blocks with DIN rails of 35 x 7,5 mm insulated mounted (without N/PE Quick-terminals)",865,5,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",66.8,CU35VMW    Compact DB 3PW 5R media WiFi,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Cable entry covers

Lock replacement parts

Sheet steel- and transparent doors

Media panels

Distribution panels

CombiLine modules"
CU36VMW,1,0,0,1,1,865,28.5,"ComfortLine Compact CU distribution boards for flush and hollow wall mounting*

with distribution panels, frames and sheet steel doors.",144,IK09,"II, insulated

I, grounded in connection with earthing set (accessories)",3,2CPX052684R9999,"DIN rail spacing 125 mm/150 mm

Fields for DIN rail devices with DIN rails of 35 x 7,5 mm and N/PE Quick-terminals (1 x ZK224 per field width)

Fields with mounting plates

Fields for terminal blocks with DIN rails of 35 x 7,5 mm insulated mounted (without N/PE Quick-terminals)",1015,6,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",77.7,CU36VMW    Compact DB 3PW 6R media WiFi,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Cable entry covers

Lock replacement parts

Sheet steel- and transparent doors

Media panels

Distribution panels

CombiLine modules"
CU14,0,0,1,1,1,365,8,"ComfortLine Compact CU distribution boards. For flush and hollow wall mounting*,

empty cabinets with blend frame and sheet steel doors.",48,IK09,"II, insulated

I, grounded in connection with earthing set (accessories)",1,2CPX052630R9999,"Prepared for expansion with CombiLine modules, distribution panels, and media panels

Without N/PE Quick-terminals",715,4,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",22.1,CU14       Comp.DB 1PW 4R empty w.door,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Hollow wall set for flush-mounted cabinets

Lock replacement parts

Media fields

Distribution panels

CombiLine modules"
CU15,0,0,1,1,1,365,9.5,"ComfortLine Compact CU distribution boards. For flush and hollow wall mounting*,

empty cabinets with blend frame and sheet steel doors.",60,IK09,"II, insulated

I, grounded in connection with earthing set (accessories)",1,2CPX052631R9999,"Prepared for expansion with CombiLine modules, distribution panels, and media panels

Without N/PE Quick-terminals",865,5,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",26.5,CU15       Comp.DB 1PW 5R empty w.door,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Hollow wall set for flush-mounted cabinets

Lock replacement parts

Media fields

Distribution panels

CombiLine modules"
CU16,0,0,1,1,1,365,11,"ComfortLine Compact CU distribution boards. For flush and hollow wall mounting*,

empty cabinets with blend frame and sheet steel doors.",72,IK09,"II, insulated

I, grounded in connection with earthing set (accessories)",1,2CPX052632R9999,"Prepared for expansion with CombiLine modules, distribution panels, and media panels

Without N/PE Quick-terminals",1015,6,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",30.9,CU16       Comp.DB 1PW 6R empty w.door,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Hollow wall set for flush-mounted cabinets

Lock replacement parts

Media fields

Distribution panels

CombiLine modules"
CU17,0,0,1,1,1,365,13,"ComfortLine Compact CU distribution boards. For flush and hollow wall mounting*,

empty cabinets with blend frame and sheet steel doors.",84,IK09,"II, insulated

I, grounded in connection with earthing set (accessories)",1,2CPX052633R9999,"Prepared for expansion with CombiLine modules, distribution panels, and media panels

Without N/PE Quick-terminals",1165,7,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",35.5,CU17       Comp.DB 1PW 7R empty w.door,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Hollow wall set for flush-mounted cabinets

Lock replacement parts

Media fields

Distribution panels

CombiLine modules"
CU18,0,0,1,1,1,365,14,"ComfortLine Compact CU distribution boards. For flush and hollow wall mounting*,

empty cabinets with blend frame and sheet steel doors.",96,IK09,"II, insulated

I, grounded in connection with earthing set (accessories)",1,2CPX052634R9999,"Prepared for expansion with CombiLine modules, distribution panels, and media panels

Without N/PE Quick-terminals",1315,8,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",39.9,CU18       Comp.DB 1PW 8R empty w.door,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Hollow wall set for flush-mounted cabinets

Lock replacement parts

Media fields

Distribution panels

CombiLine modules"
CU23,0,0,1,1,1,615,9.5,"ComfortLine Compact CU distribution boards. For flush and hollow wall mounting*,

empty cabinets with blend frame and sheet steel doors",72,IK09,"II, insulated

I, grounded in connection with earthing set (accessories)",2,2CPX052635R9999,"Prepared for expansion with CombiLine modules, distribution panels, and media panels

Without N/PE Quick-terminals",565,3,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",35.1,CU23       Comp.DB 2PW 3R empty w.door,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Hollow wall set for flush-mounted cabinets

Lock replacement parts

Media fields

Distribution panels

CombiLine modules"
CU24,0,0,1,1,1,615,12,"ComfortLine Compact CU distribution boards. For flush and hollow wall mounting*,

empty cabinets with blend frame and sheet steel doors",96,IK09,"II, insulated

I, grounded in connection with earthing set (accessories)",2,2CPX052636R9999,"Prepared for expansion with CombiLine modules, distribution panels, and media panels

Without N/PE Quick-terminals",715,4,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",36.8,CU24       Comp.DB 2PW 4R empty w.door,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Hollow wall set for flush-mounted cabinets

Lock replacement parts

Media fields

Distribution panels

CombiLine modules"
CU25,0,0,1,1,1,615,14,"ComfortLine Compact CU distribution boards. For flush and hollow wall mounting*,

empty cabinets with blend frame and sheet steel doors",120,IK09,"II, insulated

I, grounded in connection with earthing set (accessories)",2,2CPX052637R9999,"Prepared for expansion with CombiLine modules, distribution panels, and media panels

Without N/PE Quick-terminals",865,5,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",43.5,CU25       Comp.DB 2PW 5R empty w.door,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Hollow wall set for flush-mounted cabinets

Lock replacement parts

Media fields

Distribution panels

CombiLine modules"
CU26,0,0,1,1,1,615,16,"ComfortLine Compact CU distribution boards. For flush and hollow wall mounting*,

empty cabinets with blend frame and sheet steel doors",144,IK09,"II, insulated

I, grounded in connection with earthing set (accessories)",2,2CPX052638R9999,"Prepared for expansion with CombiLine modules, distribution panels, and media panels

Without N/PE Quick-terminals",1015,6,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",50.2,CU26       Comp.DB 2PW 6R empty w.door,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Hollow wall set for flush-mounted cabinets

Lock replacement parts

Media fields

Distribution panels

CombiLine modules"
CU27,0,0,1,1,1,615,18,"ComfortLine Compact CU distribution boards. For flush and hollow wall mounting*,

empty cabinets with blend frame and sheet steel doors",168,IK09,"II, insulated

I, grounded in connection with earthing set (accessories)",2,2CPX052639R9999,"Prepared for expansion with CombiLine modules, distribution panels, and media panels

Without N/PE Quick-terminals",1165,7,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",56.9,CU27       Comp.DB 2PW 7R empty w.door,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Hollow wall set for flush-mounted cabinets

Lock replacement parts

Media fields

Distribution panels

CombiLine modules"
CU28,0,0,1,1,1,615,19.5,"ComfortLine Compact CU distribution boards. For flush and hollow wall mounting*,

empty cabinets with blend frame and sheet steel doors",192,IK09,"II, insulated

I, grounded in connection with earthing set (accessories)",2,2CPX052640R9999,"Prepared for expansion with CombiLine modules, distribution panels, and media panels

Without N/PE Quick-terminals",1315,8,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",63.6,CU28       Comp.DB 2PW 8R empty w.door,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Hollow wall set for flush-mounted cabinets

Lock replacement parts

Media fields

Distribution panels

CombiLine modules"
CU34,0,0,1,1,1,865,16,"ComfortLine Compact CU distribution boards. For flush and hollow wall mounting*,

empty cabinets with blend frame and sheet steel doors",144,IK09,"II, insulated

I, grounded in connection with earthing set (accessories)",3,2CPX052641R9999,"Prepared for expansion with CombiLine modules, distribution panels, and media panels

Without N/PE Quick-terminals",715,4,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",52.7,CU34       Comp.DB 3PW 4R empty w.door,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Hollow wall set for flush-mounted cabinets

Lock replacement parts

Media fields

Distribution panels

CombiLine modules"
CU35,0,0,1,1,1,865,19,"ComfortLine Compact CU distribution boards. For flush and hollow wall mounting*,

empty cabinets with blend frame and sheet steel doors",180,IK09,"II, insulated

I, grounded in connection with earthing set (accessories)",3,2CPX052642R9999,"Prepared for expansion with CombiLine modules, distribution panels, and media panels

Without N/PE Quick-terminals",865,5,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",61.7,CU35       Comp.DB 3PW 5R empty w.door,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Hollow wall set for flush-mounted cabinets

Lock replacement parts

Media fields

Distribution panels

CombiLine modules"
CU36,0,0,1,1,1,865,22.5,"ComfortLine Compact CU distribution boards. For flush and hollow wall mounting*,

empty cabinets with blend frame and sheet steel doors",216,IK09,"II, insulated

I, grounded in connection with earthing set (accessories)",3,2CPX052643R9999,"Prepared for expansion with CombiLine modules, distribution panels, and media panels

Without N/PE Quick-terminals",1015,6,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",70.5,CU36       Comp.DB 3PW 6R empty w.door,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Hollow wall set for flush-mounted cabinets

Lock replacement parts

Media fields

Distribution panels

CombiLine modules"
CU37,0,0,1,1,1,865,24.5,"ComfortLine Compact CU distribution boards. For flush and hollow wall mounting*,

empty cabinets with blend frame and sheet steel doors",252,IK09,"II, insulated

I, grounded in connection with earthing set (accessories)",3,2CPX052644R9999,"Prepared for expansion with CombiLine modules, distribution panels, and media panels

Without N/PE Quick-terminals",1165,7,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",82.1,CU37       Comp.DB 3PW 7R empty w.door,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Hollow wall set for flush-mounted cabinets

Lock replacement parts

Media fields

Distribution panels

CombiLine modules"
CU45,0,0,1,1,1,1115,23,"ComfortLine Compact CU distribution boards. For flush and hollow wall mounting*,

empty cabinets with blend frame and sheet steel doors",240,IK09,"II, insulated

I, grounded in connection with earthing set (accessories)",4,2CPX052645R9999,"Prepared for expansion with CombiLine modules, distribution panels, and media panels

Without N/PE Quick-terminals",865,5,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",56.2,CU45       Comp.DB 4PW 5R empty w.door,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Hollow wall set for flush-mounted cabinets

Lock replacement parts

Media fields

Distribution panels

CombiLine modules"
CU46,0,0,1,1,1,1115,27,"ComfortLine Compact CU distribution boards. For flush and hollow wall mounting*,

empty cabinets with blend frame and sheet steel doors",288,IK09,"II, insulated

I, grounded in connection with earthing set (accessories)",4,2CPX052646R9999,"Prepared for expansion with CombiLine modules, distribution panels, and media panels

Without N/PE Quick-terminals",1015,6,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

120° door opening angle

From 3-field width double door cabinets

Doors with espagnolette closure

With cable pull/tension mount",63.9,CU46       Comp.DB 4PW 6R empty w.door,"Cabinet with frame and door

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,"Hollow wall set for flush-mounted cabinets

Lock replacement parts

Media fields

Distribution panels

CombiLine modules"
CU24VD,0,0,0,0,0,615,15,"ComfortLine Compact CU distribution boards.

For flush and hollow wall mounting*, with distribution panels and design frames.",96,IK09,"II, insulated",2,2CPX052687R9999,"DIN rail spacing 125 mm

Fields for DIN rail devices with DIN rails of 35 x 7,5 mm and N/PE Quick-terminals (1 x ZK224 per field width)",715,4,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

Interchangeable design frames, brushed aluminium with glass insert

120° door opening angle

Interchangeable design frame with magnetic closure

With cable pull/tension mount",36.8,CU24VD     Comp.DB 2PW 4R deco door,"Cabinet with blend frame and interchangeable design frame

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,Hollow wall set for flush-mounted cabinets
CU25VD,0,0,0,0,0,615,18,"ComfortLine Compact CU distribution boards.

For flush and hollow wall mounting*, with distribution panels and design frames.",120,IK09,"II, insulated",2,2CPX052688R9999,"DIN rail spacing 125 mm

Fields for DIN rail devices with DIN rails of 35 x 7,5 mm and N/PE Quick-terminals (1 x ZK224 per field width)",865,5,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

Interchangeable design frames, brushed aluminium with glass insert

120° door opening angle

Interchangeable design frame with magnetic closure

With cable pull/tension mount",43.5,CU25VD     Comp.DB 2PW 5R deco door,"Cabinet with blend frame and interchangeable design frame

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,Hollow wall set for flush-mounted cabinets
CU26VD,0,0,0,0,0,615,20.5,"ComfortLine Compact CU distribution boards.

For flush and hollow wall mounting*, with distribution panels and design frames.",144,IK09,"II, insulated",2,2CPX052689R9999,"DIN rail spacing 125 mm

Fields for DIN rail devices with DIN rails of 35 x 7,5 mm and N/PE Quick-terminals (1 x ZK224 per field width)",1015,6,"Galvanized steel masonry box

Made of sheet steel, color white RAL 9016, powder-coated

Interchangeable design frames, brushed aluminium with glass insert

120° door opening angle

Interchangeable design frame with magnetic closure

With cable pull/tension mount",50.2,CU26VD     Comp.DB 2PW 6R deco door,"Cabinet with blend frame and interchangeable design frame

Blend frame with 25 mm of plaster compensation

Top and bottom cable entry sliders included per field width

Labeling system included",IP30,Hollow wall set for flush-mounted cabinets
