B E I P R S T V W

## I

InitByBaudRate(PL2303Driver.BaudRate) - Method in class tw.com.prolific.driver.pl2303.PL2303Driver
  Open an PL2303HXD USB Device by BaudRate
InitByDefualtValue() - Method in class tw.com.prolific.driver.pl2303.PL2303Driver
  Open an PL2303HXD USB Device
InitByPortSetting(PL2303Driver.BaudRate, PL2303Driver.DataBits, PL2303Driver.StopBits, PL2303Driver.Parity, PL2303Driver.FlowControl) - Method in class tw.com.prolific.driver.pl2303.PL2303Driver
  Open an PL2303HXD USB Device by PortSetting
isConnected() - Method in class tw.com.prolific.driver.pl2303.PL2303Driver
  Get the connection status of this PL2303HXD, ie, whether there is an active connection with PL2303HXD device.

B E I P R S T V W