,l1##LENGTH##MILLIMETERS,connection##OTHER##,Weight##MASS##KILOGRAMS,URL##OTHER##,Product Type##OTHER##,Product Series##OTHER##,Product Name##OTHER##,Order Code##OTHER##,Nominal connection##OTHER##,Nominal1##LENGTH##MILLIMETERS,NRLS_C_code_fabrikant_gln##OTHER##,NLRS_C_model##OTHER##,NLRS_C_content_versie##OTHER##,NLRS_C_content_provider##OTHER##,NLRS_C_content_datum_uitgifte##OTHER##,NLRS_C_content_datum_gewijzigd##OTHER##,NLRS_C_content_creator##OTHER##,NLRS_C_code_gtin##OTHER##,NLRS_C_code_fabrikant_product##OTHER##,NLRS_C_code_SfB_tabel##OTHER##,NLRS_C_code_ETIM##OTHER##,NLRS_C_Revit_versie##OTHER##,ModelReference##OTHER##,ModelNumber##OTHER##,Model##OTHER##,Minimum working pressure##HVAC_PRESSURE##BARS,Maximum working pressure##HVAC_PRESSURE##BARS,Material##OTHER##,Manufacturer##OTHER##,ManufactureName##OTHER##,Kvs value (m3/h)##OTHER##,IfcExportType##OTHER##,IfcExportAs##OTHER##,GTIN##OTHER##,Flowrate (10% system flow)##PIPING_FLOW##LITERS_PER_SECOND,Flow through capacity (m3/h)##OTHER##,Fixed magnetic bars##OTHER##,Filter bag volume##PIPING_VOLUME##LITERS,ETIM Group##OTHER##,ETIM Class##OTHER##,DurationUnit##OTHER##,Description##OTHER##,CreatedOn##OTHER##,CreatedBy##OTHER##,Connection1##LENGTH##MILLIMETERS,AssetType##OTHER##,Article##OTHER##,Actual1##LENGTH##MILLIMETERS
17021-Sideflow-Clean_3.5L,468.500000000000,G 1/2 "" F,10.000000000000,www.flamcogroup.com,3.5L,SideFlow Clean Dirt Separators,SideFlow Clean,17021,1,12.700000000000,,SideFlow Clean,Versie: 1.0,Flamco Group,,,Technisch Bureau Lindhout,08712874170216,17021,,EC010260 Air-/dirt separator for central heating/cooling system,2018,,,SideFlow Clean,0.200000000000,10.000000000000,,Flamco Group,Flamco Group,17,,,08712874170216,0.800000000000,2.88,1,1.400000000000,EG015140 Filters/separators,EC010260 Air-/dirt separator for central heating/cooling system,,SideFlow Clean 3.5L,,TBL,12.700000000000,,17021,21.300000000000
