IFC building model
Schema: "IFC4"
Description: "ViewDefinition [ReferenceView_V1.2]"
File name: "0001"
Time stamp: "2024-12-16T17:33:07"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "22.0.2.392 - Exporter 22.0.2.392 - Alternate UI 22.0.2.392"
Application: "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)"

People and organizations
  Person "user" of Organization (no name given)
  Owner history of Person "user" of Organization (no name given) | application "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)" | change NOCHANGE | created 1731337144 (2024-11-11T14:59:04Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT "0001" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 31.181945″ | longitude -71° 3′ 24.263305″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "Boston", "MA"
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:8mm Head" | elevation 0.
        contains 1 element
          1 x IFCLIGHTFIXTURE | type IFCLIGHTFIXTURETYPE "Sanitary_Mirrors_DURAVIT-AG_Light-&-mirror-Mirror-cabinet-Mirrored-White-Matt-LM7841:Light & mirror Mirror cabinet Mirrored, White Matt - LM7841000000" | object type "Sanitary_Mirrors_DURAVIT-AG_Light-&-mirror-Mirror-cabinet-Mirrored-White-Matt-LM7841:Light & mirror Mirror cabinet Mirrored, White Matt - LM7841000000" | names: "Sanitary_Mirrors_DURAVIT-AG_Light-&-mirror-Mirror-cabinet-Mirrored-White-Matt-LM7841:Light & mirror Mirror cabinet Mirrored, White Matt - LM7841000000:456973" | material: constituents "MaterialConstituentSet" ("Duravit - Plastic - White": "Duravit - Plastic - White", "Duravit - Wood - M22 - White High Gloss Decor": "Duravit - Wood - M22 - White High Gloss Decor", "Duravit - Metal - Chrome": "Duravit - Metal - Chrome", "Duravit - Glass - Mirror": "Duravit - Glass - Mirror", "Duravit - Glass - Clear": "Duravit - Glass - Clear") | property sets: Pset_ElectricalDeviceCommon, Pset_EnvironmentalImpactIndicators, Pset_LightFixtureTypeCommon, Pset_ManufacturerTypeInformation, Constraints, Dimensions

Types
  IFCLIGHTFIXTURETYPE "Sanitary_Mirrors_DURAVIT-AG_Light-&-mirror-Mirror-cabinet-Mirrored-White-Matt-LM7841:Light & mirror Mirror cabinet Mirrored, White Matt - LM7841000000" | 1 occurrence | material: constituents "MaterialConstituentSet" ("Duravit - Plastic - White": "Duravit - Plastic - White", "Duravit - Wood - M22 - White High Gloss Decor": "Duravit - Wood - M22 - White High Gloss Decor", "Duravit - Metal - Chrome": "Duravit - Metal - Chrome", "Duravit - Glass - Mirror": "Duravit - Glass - Mirror", "Duravit - Glass - Clear": "Duravit - Glass - Clear") | property sets: Constraints, Dimensions, Electrical, Electrical - Loads, Identity Data, Materials and Finishes

Property sets
  Pset_SiteCommon | properties | on 1 object (1 IFCSITE)
    Reference = "Project Information" (IFCIDENTIFIER)
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCLIGHTFIXTURE)
    Mark = "4" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Date Created = "2024/11/08" (IFCTEXT)
    Date Updated = "" (IFCTEXT)
    Description = "Duravit Light & mirror Mirror cabinet, White, Version: Best, Number of doors: 2, Hinge position: Left, Right, Mirror surfaces: Double mirror doors, Back panel mirror, Number of glass shelves: 2, Body material: Glass, Highly compressed three-layer chipboard, 15 W, Turn on lighting: Switch Inside, Bottom, Right, Socket: Integrated, Number of sockets: 1, plug socket type: F, 4000 K, LED light for washing area: Integrated, Service life of illuminant: > 30000 h, Replaceable illuminant: No, Energy efficiency class D - LM7841000000" (IFCTEXT)
    Installation instructions = "" (IFCTEXT)
    Manufacturer = "Duravit" (IFCTEXT)
    Model = "Light & mirror Mirror cabinet Mirrored, White Matt - LM7841" (IFCTEXT)
    OmniClass Number = "23.21.37.13.15" (IFCTEXT)
    OmniClass Title = "Mirrors" (IFCTEXT)
    Product Documentation Link = "https://pro.duravit.com/" (IFCTEXT)
    Product Page URL = "https://pro.duravit.com/p/LM7841" (IFCTEXT)
    Product certification = "" (IFCTEXT)
    Product data url = "https://bimobject.com/duravit/product/light-mirror-mirror-cabinet-mirrored-white-matt-lm7841" (IFCTEXT)
    Type Name = "Light & mirror Mirror cabinet Mirrored, White Matt - LM7841000000" (IFCTEXT)
    URL = "http://pro.duravit.com" (IFCTEXT)
    Version = 1 (IFCINTEGER)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Owner" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "0001" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other | properties | on 1 object (1 IFCLIGHTFIXTURE)
    Category = "Lighting Fixtures" (IFCLABEL)
    Family = "Sanitary_Mirrors_DURAVIT-AG_Light-&-mirror-Mirror-cabinet-Mirrored-White-Matt-LM7841: Light & mirror Mirror cabinet Mirrored, White Matt - LM7841000000" (IFCLABEL)
    Family and Type = "Sanitary_Mirrors_DURAVIT-AG_Light-&-mirror-Mirror-cabinet-Mirrored-White-Matt-LM7841: Light & mirror Mirror cabinet Mirrored, White Matt - LM7841000000" (IFCLABEL)
    Type = "Sanitary_Mirrors_DURAVIT-AG_Light-&-mirror-Mirror-cabinet-Mirrored-White-Matt-LM7841: Light & mirror Mirror cabinet Mirrored, White Matt - LM7841000000" (IFCLABEL)
    Type Id = "Sanitary_Mirrors_DURAVIT-AG_Light-&-mirror-Mirror-cabinet-Mirrored-White-Matt-LM7841: Light & mirror Mirror cabinet Mirrored, White Matt - LM7841000000" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: 8mm Head" (IFCLABEL)
    Family and Type = "Level: 8mm Head" (IFCLABEL)
    Type = "Level: 8mm Head" (IFCLABEL)
    Type Id = "Level: 8mm Head" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Lighting Fixtures" (IFCLABEL)
    Family Name = "Sanitary_Mirrors_DURAVIT-AG_Light-&-mirror-Mirror-cabinet-Mirrored-White-Matt-LM7841" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Pset_ElectricalDeviceCommon | properties | on 1 object (1 IFCLIGHTFIXTURE) | on 1 type object
    NumberOfPoles = 1 (IFCINTEGER)
    PowerFactor = 1. (IFCNORMALISEDRATIOMEASURE)
  Pset_EnvironmentalImpactIndicators | properties | on 1 object (1 IFCLIGHTFIXTURE)
    Reference = "Sanitary_Mirrors_DURAVIT-AG_Light-&-mirror-Mirror-cabinet-Mirrored-White-Matt-LM7841:Light & mirror Mirror cabinet Mirrored, White Matt - LM7841000000" (IFCIDENTIFIER)
  Pset_LightFixtureTypeCommon | properties | on 1 object (1 IFCLIGHTFIXTURE)
    Reference = "Sanitary_Mirrors_DURAVIT-AG_Light-&-mirror-Mirror-cabinet-Mirrored-White-Matt-LM7841:Light & mirror Mirror cabinet Mirrored, White Matt - LM7841000000" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCLIGHTFIXTURE) | on 1 type object
    Manufacturer = "Duravit" (IFCLABEL)
  Constraints | properties | on 1 object (1 IFCLIGHTFIXTURE)
    Elevation from Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
    Schedule Level = "Level: Level 1" (IFCLABEL)
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 type object
    Default Elevation = 1200. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCLIGHTFIXTURE)
    Area = 3.41035479316112 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.215492866972561 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 type object
    Depth = 148. (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 760. (IFCLENGTHMEASURE) [MILLI METRE]
    Light Source Symbol Size = 609.6 (IFCLENGTHMEASURE) [MILLI METRE]
    Weight = 26. (IFCMASSMEASURE) [KILO GRAM]
    Width = 810. (IFCLENGTHMEASURE) [MILLI METRE]
  Electrical - Circuiting | properties | on 1 object (1 IFCLIGHTFIXTURE)
    Electrical Data = "Electrical connector 220-240V 230 V/1-230 VA" (IFCTEXT)
  Electrical - Lighting | properties | on 1 object (1 IFCLIGHTFIXTURE)
    Calculate Coefficient of Utilization = FALSE (IFCBOOLEAN)
  Electrical - Loads | properties | on 1 object (1 IFCLIGHTFIXTURE)
    Circuit Number = "" (IFCTEXT)
    Panel = "" (IFCTEXT)
  Electrical - Loads | properties | on 1 type object
    Apparent Load = 230. (IFCPOWERMEASURE) [WATT]
  Phasing | properties | on 1 object (1 IFCLIGHTFIXTURE)
    Phase Created = "New Construction" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
    Reference = "Level:8mm Head" (IFCIDENTIFIER)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDING)
    AboveGround = UNKNOWN (IFCLOGICAL)
    Reference = "Project Information" (IFCIDENTIFIER)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
    Reference = "Project Information" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDING)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Project Information" (IFCIDENTIFIER)
  Pset_BuildingSystemCommon | properties | on 1 object (1 IFCBUILDING)
    Reference = "Project Information" (IFCIDENTIFIER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Level Head - Circle: M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "8mm Head" (IFCTEXT)
  Electrical | properties | on 1 type object
    Current = 1. (IFCELECTRICCURRENTMEASURE) [AMPERE]
    Number of Poles = 1 (IFCINTEGER)
    Power Factor = 1. (IFCREAL)
    Voltage = 230. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
  Materials and Finishes | properties | on 1 type object
    Material 1 = "Duravit - Wood - M22 - White High Gloss Decor" (IFCLABEL)
  Photometrics | properties | on 1 type object
    Color Filter = 16777215 (IFCINTEGER)
    Dimming Lamp Color Temperature Shift = "<None>" (IFCIDENTIFIER)
    Efficacy = 148.541963750594 (IFCREAL) [derived "Luminous Efficacy"]
    Emit Shape Visible in Rendering = FALSE (IFCBOOLEAN)
    Emit from Rectangle Length = 797. (IFCLENGTHMEASURE) [MILLI METRE]
    Emit from Rectangle Width = 60. (IFCLENGTHMEASURE) [MILLI METRE]
    Illuminance = 76.3414882467275 (IFCILLUMINANCEMEASURE) [LUX]
    Initial Color = 0 (IFCINTEGER)
    Initial Color Temperature = 4000. (IFCREAL) [KELVIN]
    Initial Intensity = 0 (IFCINTEGER)
    Light Loss Factor = 0 (IFCINTEGER)
    Light Source Definition (family) = "Rectangle+HemiSpherical" (IFCTEXT)
    Luminous Flux = 2228.12945625891 (IFCLUMINOUSFLUXMEASURE) [LUMEN]
    Luminous Intensity = 709.235633624526 (IFCLUMINOUSINTENSITYMEASURE) [CANDELA]
    Total Light Loss Factor = 1. (IFCREAL)
    Wattage = 15. (IFCPOWERMEASURE) [WATT]