, EAN##OTHER##, Nominal Wattage##ELECTRICAL_WATTAGE##WATTS, Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS, Color Temperature##COLOR_TEMPERATURE##KELVIN, Cut out width##LENGTH##MILLIMETERS, CCT Switch Information##OTHER##, Model##OTHER##, URL##OTHER##, GEO##OTHER##, IES Light Source##OTHER##
DL SLIM ALU D100 V 8W MS 840 WT, 4099854441776, 8, 800, 4000, 56, This luminaire has switchable parameters ( 4000K/3000K 800lm/600lm/400lm 8W/6W/4W), DOWNLIGHT SLIM ALU D100 V 8W MS 840 WT, https://www.ledvance.com/professional/search?query=4099854441776, DL SLIM ALU D100 8W, IES_DATA_DL_SLIM_ALU : DL SLIM ALU D100 V 8W MS 840 WT
DL SLIM ALU D150 V 13W MS 840 WT, 4099854441790, 13, 1300, 4000, 81, This luminaire has switchable parameters ( 4000K/3000K 1300lm/980lm/650lm 13W/9.8W/6.5W), DOWNLIGHT SLIM ALU D150 V 13W MS 840 WT , https://www.ledvance.com/professional/search?query=4099854441790, DL SLIM ALU D150 13W, IES_DATA_DL_SLIM_ALU : DL SLIM ALU D150 V 13W MS 840 WT
DL SLIM ALU D205 V 19W MS 840 WT, 4099854441844, 19, 1900, 4000, 108.5, This luminaire has switchable parameters ( 4000K/3000K 1900lm/1430lm/950lm 19W/14.3W/9.5W), DOWNLIGHT SLIM ALU D205 V 19W MS 840 WT, https://www.ledvance.com/professional/search?query=4099854441844, DL SLIM ALU D205 19W, IES_DATA_DL_SLIM_ALU : DL SLIM ALU D205 V 19W MS 840 WT
DL SLIM ALU D175 V 16W MS 840 WT, 4099854441813, 16, 1600, 4000, 93.5, This luminaire has switchable parameters ( 4000K/3000K 1600lm/1200lm/800lm 16W/12W/8W), DOWNLIGHT SLIM ALU D175 V 16W MS 840 WT, https://www.ledvance.com/professional/search?query=4099854441813, DL SLIM ALU D175 16W, IES_DATA_DL_SLIM_ALU : DL SLIM ALU D175 V 16W MS 840 WT
DL SLIM ALU D280 V 25W MS 840 WT, 4099854441868, 25, 2500, 4000, 146, This luminaire has switchable parameters ( 4000K/3000K 2500lm/1880lm/1250lm 25W/18.8W/12.5W), DOWNLIGHT SLIM ALU D280 V 25W MS 840 WT, https://www.ledvance.com/professional/search?query=4099854441868, DL SLIM ALU D280 25W, IES_DATA_DL_SLIM_ALU : DL SLIM ALU D280 V 25W MS 840 WT
